From b3dd6876cdd40346cc7282955b8cc31401cffb31 Mon Sep 17 00:00:00 2001
From: Chengwen Feng <fengchengwen@huawei.com>
Date: Wed, 9 Oct 2024 04:50:29 +0000
Subject: [PATCH] net/tap: use new kvargs process API

[ upstream commit 4ed306131f85ef180589169b868f292d9149b0c7 ]

Some kvargs could be key=value or only-key, it should use
rte_kvargs_process_opt() instead of rte_kvargs_process() to handle
these kvargs.

Signed-off-by: Chengwen Feng <fengchengwen@huawei.com>
---
 drivers/net/tap/rte_eth_tap.c | 10 +++++-----
 1 file changed, 5 insertions(+), 5 deletions(-)

diff --git a/drivers/net/tap/rte_eth_tap.c b/drivers/net/tap/rte_eth_tap.c
index b41fa97..cdb52cf 100644
--- a/drivers/net/tap/rte_eth_tap.c
+++ b/drivers/net/tap/rte_eth_tap.c
@@ -2292,7 +2292,7 @@ rte_pmd_tun_probe(struct rte_vdev_device *dev)
 		kvlist = rte_kvargs_parse(params, valid_arguments);
 		if (kvlist) {
 			if (rte_kvargs_count(kvlist, ETH_TAP_IFACE_ARG) == 1) {
-				ret = rte_kvargs_process(kvlist,
+				ret = rte_kvargs_process_opt(kvlist,
 					ETH_TAP_IFACE_ARG,
 					&set_interface_name,
 					tun_name);
@@ -2496,10 +2496,10 @@ rte_pmd_tap_probe(struct rte_vdev_device *dev)
 		kvlist = rte_kvargs_parse(params, valid_arguments);
 		if (kvlist) {
 			if (rte_kvargs_count(kvlist, ETH_TAP_IFACE_ARG) == 1) {
-				ret = rte_kvargs_process(kvlist,
-							 ETH_TAP_IFACE_ARG,
-							 &set_interface_name,
-							 tap_name);
+				ret = rte_kvargs_process_opt(kvlist,
+							     ETH_TAP_IFACE_ARG,
+							     &set_interface_name,
+							     tap_name);
 				if (ret == -1)
 					goto leave;
 			}
-- 
2.33.0

