From f8e2db6965abc49f6f9c80df2b8277969cec2988 Mon Sep 17 00:00:00 2001
From: Chengwen Feng <fengchengwen@huawei.com>
Date: Fri, 12 Jan 2024 10:26:59 +0000
Subject: [PATCH 15/30] dmadev: add tracepoints in data path API
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

[ upstream commit 112327c220befef14129e4852e8df46e60410128 ]

Add tracepoints at data path APIs for tracing support.

Signed-off-by: Chengwen Feng <fengchengwen@huawei.com>
Acked-by: Morten Brørup <mb@smartsharesystems.com>
---
 lib/dmadev/meson.build               |   2 +-
 lib/dmadev/rte_dmadev.h              |  56 +++++++---
 lib/dmadev/rte_dmadev_trace_fp.h     | 150 +++++++++++++++++++++++++++
 lib/dmadev/rte_dmadev_trace_points.c |  27 +++++
 lib/dmadev/version.map               |  15 +++
 5 files changed, 236 insertions(+), 14 deletions(-)
 create mode 100644 lib/dmadev/rte_dmadev_trace_fp.h

diff --git a/lib/dmadev/meson.build b/lib/dmadev/meson.build
index e0d90ae..62b0650 100644
--- a/lib/dmadev/meson.build
+++ b/lib/dmadev/meson.build
@@ -3,7 +3,7 @@
 
 sources = files('rte_dmadev.c', 'rte_dmadev_trace_points.c')
 headers = files('rte_dmadev.h')
-indirect_headers += files('rte_dmadev_core.h')
+indirect_headers += files('rte_dmadev_core.h', 'rte_dmadev_trace_fp.h')
 driver_sdk_headers += files('rte_dmadev_pmd.h')
 
 deps += ['telemetry']
diff --git a/lib/dmadev/rte_dmadev.h b/lib/dmadev/rte_dmadev.h
index 450b81c..5474a52 100644
--- a/lib/dmadev/rte_dmadev.h
+++ b/lib/dmadev/rte_dmadev.h
@@ -773,6 +773,7 @@ struct rte_dma_sge {
 };
 
 #include "rte_dmadev_core.h"
+#include "rte_dmadev_trace_fp.h"
 
 /**@{@name DMA operation flag
  * @see rte_dma_copy()
@@ -836,6 +837,7 @@ rte_dma_copy(int16_t dev_id, uint16_t vchan, rte_iova_t src, rte_iova_t dst,
 	     uint32_t length, uint64_t flags)
 {
 	struct rte_dma_fp_object *obj = &rte_dma_fp_objs[dev_id];
+	int ret;
 
 #ifdef RTE_DMADEV_DEBUG
 	if (!rte_dma_is_valid(dev_id) || length == 0)
@@ -844,7 +846,10 @@ rte_dma_copy(int16_t dev_id, uint16_t vchan, rte_iova_t src, rte_iova_t dst,
 		return -ENOTSUP;
 #endif
 
-	return (*obj->copy)(obj->dev_private, vchan, src, dst, length, flags);
+	ret = (*obj->copy)(obj->dev_private, vchan, src, dst, length, flags);
+	rte_dma_trace_copy(dev_id, vchan, src, dst, length, flags, ret);
+
+	return ret;
 }
 
 /**
@@ -883,6 +888,7 @@ rte_dma_copy_sg(int16_t dev_id, uint16_t vchan, struct rte_dma_sge *src,
 		uint64_t flags)
 {
 	struct rte_dma_fp_object *obj = &rte_dma_fp_objs[dev_id];
+	int ret;
 
 #ifdef RTE_DMADEV_DEBUG
 	if (!rte_dma_is_valid(dev_id) || src == NULL || dst == NULL ||
@@ -892,8 +898,12 @@ rte_dma_copy_sg(int16_t dev_id, uint16_t vchan, struct rte_dma_sge *src,
 		return -ENOTSUP;
 #endif
 
-	return (*obj->copy_sg)(obj->dev_private, vchan, src, dst, nb_src,
-			       nb_dst, flags);
+	ret = (*obj->copy_sg)(obj->dev_private, vchan, src, dst, nb_src,
+			      nb_dst, flags);
+	rte_dma_trace_copy_sg(dev_id, vchan, src, dst, nb_src, nb_dst, flags,
+			      ret);
+
+	return ret;
 }
 
 /**
@@ -927,6 +937,7 @@ rte_dma_fill(int16_t dev_id, uint16_t vchan, uint64_t pattern,
 	     rte_iova_t dst, uint32_t length, uint64_t flags)
 {
 	struct rte_dma_fp_object *obj = &rte_dma_fp_objs[dev_id];
+	int ret;
 
 #ifdef RTE_DMADEV_DEBUG
 	if (!rte_dma_is_valid(dev_id) || length == 0)
@@ -935,8 +946,11 @@ rte_dma_fill(int16_t dev_id, uint16_t vchan, uint64_t pattern,
 		return -ENOTSUP;
 #endif
 
-	return (*obj->fill)(obj->dev_private, vchan, pattern, dst, length,
-			    flags);
+	ret = (*obj->fill)(obj->dev_private, vchan, pattern, dst, length,
+			   flags);
+	rte_dma_trace_fill(dev_id, vchan, pattern, dst, length, flags, ret);
+
+	return ret;
 }
 
 /**
@@ -957,6 +971,7 @@ static inline int
 rte_dma_submit(int16_t dev_id, uint16_t vchan)
 {
 	struct rte_dma_fp_object *obj = &rte_dma_fp_objs[dev_id];
+	int ret;
 
 #ifdef RTE_DMADEV_DEBUG
 	if (!rte_dma_is_valid(dev_id))
@@ -965,7 +980,10 @@ rte_dma_submit(int16_t dev_id, uint16_t vchan)
 		return -ENOTSUP;
 #endif
 
-	return (*obj->submit)(obj->dev_private, vchan);
+	ret = (*obj->submit)(obj->dev_private, vchan);
+	rte_dma_trace_submit(dev_id, vchan, ret);
+
+	return ret;
 }
 
 /**
@@ -995,7 +1013,7 @@ rte_dma_completed(int16_t dev_id, uint16_t vchan, const uint16_t nb_cpls,
 		  uint16_t *last_idx, bool *has_error)
 {
 	struct rte_dma_fp_object *obj = &rte_dma_fp_objs[dev_id];
-	uint16_t idx;
+	uint16_t idx, ret;
 	bool err;
 
 #ifdef RTE_DMADEV_DEBUG
@@ -1019,8 +1037,12 @@ rte_dma_completed(int16_t dev_id, uint16_t vchan, const uint16_t nb_cpls,
 		has_error = &err;
 
 	*has_error = false;
-	return (*obj->completed)(obj->dev_private, vchan, nb_cpls, last_idx,
-				 has_error);
+	ret = (*obj->completed)(obj->dev_private, vchan, nb_cpls, last_idx,
+				has_error);
+	rte_dma_trace_completed(dev_id, vchan, nb_cpls, last_idx, has_error,
+				ret);
+
+	return ret;
 }
 
 /**
@@ -1055,7 +1077,7 @@ rte_dma_completed_status(int16_t dev_id, uint16_t vchan,
 			 enum rte_dma_status_code *status)
 {
 	struct rte_dma_fp_object *obj = &rte_dma_fp_objs[dev_id];
-	uint16_t idx;
+	uint16_t idx, ret;
 
 #ifdef RTE_DMADEV_DEBUG
 	if (!rte_dma_is_valid(dev_id) || nb_cpls == 0 || status == NULL)
@@ -1067,8 +1089,12 @@ rte_dma_completed_status(int16_t dev_id, uint16_t vchan,
 	if (last_idx == NULL)
 		last_idx = &idx;
 
-	return (*obj->completed_status)(obj->dev_private, vchan, nb_cpls,
-					last_idx, status);
+	ret = (*obj->completed_status)(obj->dev_private, vchan, nb_cpls,
+				       last_idx, status);
+	rte_dma_trace_completed_status(dev_id, vchan, nb_cpls, last_idx, status,
+				       ret);
+
+	return ret;
 }
 
 /**
@@ -1087,6 +1113,7 @@ static inline uint16_t
 rte_dma_burst_capacity(int16_t dev_id, uint16_t vchan)
 {
 	struct rte_dma_fp_object *obj = &rte_dma_fp_objs[dev_id];
+	uint16_t ret;
 
 #ifdef RTE_DMADEV_DEBUG
 	if (!rte_dma_is_valid(dev_id))
@@ -1094,7 +1121,10 @@ rte_dma_burst_capacity(int16_t dev_id, uint16_t vchan)
 	if (*obj->burst_capacity == NULL)
 		return 0;
 #endif
-	return (*obj->burst_capacity)(obj->dev_private, vchan);
+	ret = (*obj->burst_capacity)(obj->dev_private, vchan);
+	rte_dma_trace_burst_capacity(dev_id, vchan, ret);
+
+	return ret;
 }
 
 #ifdef __cplusplus
diff --git a/lib/dmadev/rte_dmadev_trace_fp.h b/lib/dmadev/rte_dmadev_trace_fp.h
new file mode 100644
index 0000000..f5b9683
--- /dev/null
+++ b/lib/dmadev/rte_dmadev_trace_fp.h
@@ -0,0 +1,150 @@
+/* SPDX-License-Identifier: BSD-3-Clause
+ * Copyright(c) 2024 HiSilicon Limited
+ */
+
+#ifndef RTE_DMADEV_TRACE_FP_H
+#define RTE_DMADEV_TRACE_FP_H
+
+/**
+ * @file
+ *
+ * API for dmadev fastpath trace support
+ */
+
+#include <rte_trace_point.h>
+
+#ifdef __cplusplus
+extern "C" {
+#endif
+
+RTE_TRACE_POINT_FP(
+	rte_dma_trace_stats_get,
+	RTE_TRACE_POINT_ARGS(int16_t dev_id, uint16_t vchan,
+			     struct rte_dma_stats *stats, int ret),
+	rte_trace_point_emit_i16(dev_id);
+	rte_trace_point_emit_u16(vchan);
+	rte_trace_point_emit_u64(stats->submitted);
+	rte_trace_point_emit_u64(stats->completed);
+	rte_trace_point_emit_u64(stats->errors);
+	rte_trace_point_emit_int(ret);
+)
+
+RTE_TRACE_POINT_FP(
+	rte_dma_trace_vchan_status,
+	RTE_TRACE_POINT_ARGS(int16_t dev_id, uint16_t vchan,
+			     enum rte_dma_vchan_status *status, int ret),
+#ifdef _RTE_TRACE_POINT_REGISTER_H_
+	enum rte_dma_vchan_status __status = 0;
+	status = &__status;
+#endif /* _RTE_TRACE_POINT_REGISTER_H_ */
+	int vchan_status = *status;
+	rte_trace_point_emit_i16(dev_id);
+	rte_trace_point_emit_u16(vchan);
+	rte_trace_point_emit_int(vchan_status);
+	rte_trace_point_emit_int(ret);
+)
+
+RTE_TRACE_POINT_FP(
+	rte_dma_trace_copy,
+	RTE_TRACE_POINT_ARGS(int16_t dev_id, uint16_t vchan, rte_iova_t src,
+			     rte_iova_t dst, uint32_t length, uint64_t flags,
+			     int ret),
+	rte_trace_point_emit_i16(dev_id);
+	rte_trace_point_emit_u16(vchan);
+	rte_trace_point_emit_u64(src);
+	rte_trace_point_emit_u64(dst);
+	rte_trace_point_emit_u32(length);
+	rte_trace_point_emit_u64(flags);
+	rte_trace_point_emit_int(ret);
+)
+
+RTE_TRACE_POINT_FP(
+	rte_dma_trace_copy_sg,
+	RTE_TRACE_POINT_ARGS(int16_t dev_id, uint16_t vchan,
+			     struct rte_dma_sge *src, struct rte_dma_sge *dst,
+			     uint16_t nb_src, uint16_t nb_dst, uint64_t flags,
+			     int ret),
+	rte_trace_point_emit_i16(dev_id);
+	rte_trace_point_emit_u16(vchan);
+	rte_trace_point_emit_ptr(src);
+	rte_trace_point_emit_ptr(dst);
+	rte_trace_point_emit_u16(nb_src);
+	rte_trace_point_emit_u16(nb_dst);
+	rte_trace_point_emit_u64(flags);
+	rte_trace_point_emit_int(ret);
+)
+
+RTE_TRACE_POINT_FP(
+	rte_dma_trace_fill,
+	RTE_TRACE_POINT_ARGS(int16_t dev_id, uint16_t vchan, uint64_t pattern,
+			     rte_iova_t dst, uint32_t length, uint64_t flags,
+			     int ret),
+	rte_trace_point_emit_i16(dev_id);
+	rte_trace_point_emit_u16(vchan);
+	rte_trace_point_emit_u64(pattern);
+	rte_trace_point_emit_u64(dst);
+	rte_trace_point_emit_u32(length);
+	rte_trace_point_emit_u64(flags);
+	rte_trace_point_emit_int(ret);
+)
+
+RTE_TRACE_POINT_FP(
+	rte_dma_trace_submit,
+	RTE_TRACE_POINT_ARGS(int16_t dev_id, uint16_t vchan, int ret),
+	rte_trace_point_emit_i16(dev_id);
+	rte_trace_point_emit_u16(vchan);
+	rte_trace_point_emit_int(ret);
+)
+
+RTE_TRACE_POINT_FP(
+	rte_dma_trace_completed,
+	RTE_TRACE_POINT_ARGS(int16_t dev_id, uint16_t vchan,
+			     const uint16_t nb_cpls, uint16_t *last_idx,
+			     bool *has_error, uint16_t ret),
+#ifdef _RTE_TRACE_POINT_REGISTER_H_
+	uint16_t __last_idx = 0;
+	bool __has_error = false;
+	last_idx = &__last_idx;
+	has_error = &__has_error;
+#endif /* _RTE_TRACE_POINT_REGISTER_H_ */
+	int has_error_val = *has_error;
+	int last_idx_val = *last_idx;
+	rte_trace_point_emit_i16(dev_id);
+	rte_trace_point_emit_u16(vchan);
+	rte_trace_point_emit_u16(nb_cpls);
+	rte_trace_point_emit_int(last_idx_val);
+	rte_trace_point_emit_int(has_error_val);
+	rte_trace_point_emit_u16(ret);
+)
+
+RTE_TRACE_POINT_FP(
+	rte_dma_trace_completed_status,
+	RTE_TRACE_POINT_ARGS(int16_t dev_id, uint16_t vchan,
+			     const uint16_t nb_cpls, uint16_t *last_idx,
+			     enum rte_dma_status_code *status, uint16_t ret),
+#ifdef _RTE_TRACE_POINT_REGISTER_H_
+	uint16_t __last_idx = 0;
+	last_idx = &__last_idx;
+#endif /* _RTE_TRACE_POINT_REGISTER_H_ */
+	int last_idx_val = *last_idx;
+	rte_trace_point_emit_i16(dev_id);
+	rte_trace_point_emit_u16(vchan);
+	rte_trace_point_emit_u16(nb_cpls);
+	rte_trace_point_emit_int(last_idx_val);
+	rte_trace_point_emit_ptr(status);
+	rte_trace_point_emit_u16(ret);
+)
+
+RTE_TRACE_POINT_FP(
+	rte_dma_trace_burst_capacity,
+	RTE_TRACE_POINT_ARGS(int16_t dev_id, uint16_t vchan, uint16_t ret),
+	rte_trace_point_emit_i16(dev_id);
+	rte_trace_point_emit_u16(vchan);
+	rte_trace_point_emit_u16(ret);
+)
+
+#ifdef __cplusplus
+}
+#endif
+
+#endif /* RTE_DMADEV_TRACE_FP_H */
diff --git a/lib/dmadev/rte_dmadev_trace_points.c b/lib/dmadev/rte_dmadev_trace_points.c
index 2a83b90..4c74356 100644
--- a/lib/dmadev/rte_dmadev_trace_points.c
+++ b/lib/dmadev/rte_dmadev_trace_points.c
@@ -24,8 +24,35 @@ RTE_TRACE_POINT_REGISTER(rte_dma_trace_close,
 RTE_TRACE_POINT_REGISTER(rte_dma_trace_vchan_setup,
 	lib.dmadev.vchan_setup)
 
+RTE_TRACE_POINT_REGISTER(rte_dma_trace_stats_get,
+	lib.dmadev.stats_get)
+
 RTE_TRACE_POINT_REGISTER(rte_dma_trace_stats_reset,
 	lib.dmadev.stats_reset)
 
+RTE_TRACE_POINT_REGISTER(rte_dma_trace_vchan_status,
+	lib.dmadev.vchan_status)
+
 RTE_TRACE_POINT_REGISTER(rte_dma_trace_dump,
 	lib.dmadev.dump)
+
+RTE_TRACE_POINT_REGISTER(rte_dma_trace_copy,
+	lib.dmadev.copy)
+
+RTE_TRACE_POINT_REGISTER(rte_dma_trace_copy_sg,
+	lib.dmadev.copy_sg)
+
+RTE_TRACE_POINT_REGISTER(rte_dma_trace_fill,
+	lib.dmadev.fill)
+
+RTE_TRACE_POINT_REGISTER(rte_dma_trace_submit,
+	lib.dmadev.submit)
+
+RTE_TRACE_POINT_REGISTER(rte_dma_trace_completed,
+	lib.dmadev.completed)
+
+RTE_TRACE_POINT_REGISTER(rte_dma_trace_completed_status,
+	lib.dmadev.completed_status)
+
+RTE_TRACE_POINT_REGISTER(rte_dma_trace_burst_capacity,
+	lib.dmadev.burst_capacity)
diff --git a/lib/dmadev/version.map b/lib/dmadev/version.map
index 2a37365..14e0927 100644
--- a/lib/dmadev/version.map
+++ b/lib/dmadev/version.map
@@ -20,6 +20,21 @@ DPDK_24 {
 	local: *;
 };
 
+EXPERIMENTAL {
+	global:
+
+	# added in 24.03
+	__rte_dma_trace_burst_capacity;
+	__rte_dma_trace_completed;
+	__rte_dma_trace_completed_status;
+	__rte_dma_trace_copy;
+	__rte_dma_trace_copy_sg;
+	__rte_dma_trace_fill;
+	__rte_dma_trace_submit;
+
+	local: *;
+};
+
 INTERNAL {
 	global:
 
-- 
2.33.0

