From 481f0a191fc03e79bbb52b08c1d4890b6331e68d Mon Sep 17 00:00:00 2001
From: Ashish Kalra <ashish.kalra@amd.com>
Date: Tue, 5 Apr 2022 16:26:02 +0000
Subject: [PATCH 3/9] OvmfPkg/BaseMemEncryptLib: Invoke page encryption state
 change hypercall

cherry-picked from https://patchew.org/EDK2/cover.1629380011.git.ashish.kalra@amd.com .

Invoke the hypercall API to notify hypervisor when the page's
encryption state changes.

Cc: Jordan Justen <jordan.l.justen@intel.com>
Cc: Ard Biesheuvel <ard.biesheuvel@arm.com>
Signed-off-by: Brijesh Singh <brijesh.singh@amd.com>
Signed-off-by: Ashish Kalra <ashish.kalra@amd.com>
---
 .../X64/PeiDxeVirtualMemory.c                    | 16 ++++++++++++++++
 1 file changed, 16 insertions(+)

diff --git a/OvmfPkg/Library/BaseMemEncryptSevLib/X64/PeiDxeVirtualMemory.c b/OvmfPkg/Library/BaseMemEncryptSevLib/X64/PeiDxeVirtualMemory.c
index a49cf125..42e3b03f 100644
--- a/OvmfPkg/Library/BaseMemEncryptSevLib/X64/PeiDxeVirtualMemory.c
+++ b/OvmfPkg/Library/BaseMemEncryptSevLib/X64/PeiDxeVirtualMemory.c
@@ -727,6 +727,7 @@ SetMemoryEncDec (
   UINT64                          PgTableMask;
   UINT64                          AddressEncMask;
   BOOLEAN                         IsWpEnabled;
+  BOOLEAN                         CBitChanged;
   UINTN                           OrigLength;
   RETURN_STATUS                   Status;
   PHYSICAL_ADDRESS                PageAddress;
@@ -800,6 +801,7 @@ SetMemoryEncDec (
   // Save the specified length and physical address (we need it later).
   //
   OrigLength          = Length;
+  CBitChanged         = FALSE;
   OrigPhysicalAddress = PhysicalAddress;
 
   while (Length != 0) {
@@ -860,6 +862,7 @@ SetMemoryEncDec (
           ));
         PhysicalAddress += BIT30;
         Length          -= BIT30;
+        CBitChanged      = TRUE;
       } else {
         //
         // We must split the page
@@ -915,6 +918,7 @@ SetMemoryEncDec (
           SetOrClearCBit (&PageDirectory2MEntry->Uint64, Mode);
           PhysicalAddress += BIT21;
           Length          -= BIT21;
+          CBitChanged      = TRUE;
         } else {
           //
           // We must split up this page into 4K pages
@@ -958,6 +962,7 @@ SetMemoryEncDec (
         SetOrClearCBit (&PageTableEntry->Uint64, Mode);
         PhysicalAddress += EFI_PAGE_SIZE;
         Length          -= EFI_PAGE_SIZE;
+        CBitChanged      = TRUE;
       }
     }
   }
@@ -990,6 +995,17 @@ SetMemoryEncDec (
       );
   }
 
+  //
+  // Notify Hypervisor on C-bit status
+  //
+  if (CBitChanged) {
+    Status = SetMemoryEncDecHypercall3 (
+               OrigPhysicalAddress,
+               EFI_SIZE_TO_PAGES (OrigLength),
+               (Mode == SetCBit) ? TRUE : FALSE
+               );
+  }
+
 Done:
   //
   // Restore page table write protection, if any.
-- 
2.25.1

