From 6374dceef2bf72456144184cb70bdd216a744d61 Mon Sep 17 00:00:00 2001
From: May <mayshao-oc@zhaoxin.com>
Date: Wed, 15 Jan 2025 10:42:33 +0800
Subject: [PATCH 3/3] x86: Set default non_temporal_threshold for Zhaoxin
 processors

Current 'non_temporal_threshold' set to 'non_temporal_threshold_lowbound'
on Zhaoxin processors without ERMS. The default
'non_temporal_threshold_lowbound' is too small for the KH-40000 and KX-7000
Zhaoxin processors, this patch updates the value to
'shared / cachesize_non_temporal_divisor'.

Signed-off-by: May <mayshao-oc@zhaoxin.com>
---
 sysdeps/x86/cpu-features.c | 1 +
 sysdeps/x86/dl-cacheinfo.h | 6 ++++--
 2 files changed, 5 insertions(+), 2 deletions(-)

diff --git a/sysdeps/x86/cpu-features.c b/sysdeps/x86/cpu-features.c
index 43b5f562..f752ebd2 100644
--- a/sysdeps/x86/cpu-features.c
+++ b/sysdeps/x86/cpu-features.c
@@ -949,6 +949,7 @@ https://www.intel.com/content/www/us/en/support/articles/000059422/processors.ht
 
 	      /* Yongfeng and Shijidadao mircoarch tuning.  */
 	    case 0x5b:
+	      cpu_features->cachesize_non_temporal_divisor = 2;
 	    case 0x6b:
 	      cpu_features->preferred[index_arch_AVX_Fast_Unaligned_Load]
 		  &= ~bit_arch_AVX_Fast_Unaligned_Load;
diff --git a/sysdeps/x86/dl-cacheinfo.h b/sysdeps/x86/dl-cacheinfo.h
index 6c774042..bd2a9122 100644
--- a/sysdeps/x86/dl-cacheinfo.h
+++ b/sysdeps/x86/dl-cacheinfo.h
@@ -940,8 +940,10 @@ dl_init_cacheinfo (struct cpu_features *cpu_features)
   /* If no ERMS, we use the per-thread L3 chunking. Normal cacheable stores run
      a higher risk of actually thrashing the cache as they don't have a HW LRU
      hint. As well, their performance in highly parallel situations is
-     noticeably worse.  */
-  if (!CPU_FEATURE_USABLE_P (cpu_features, ERMS))
+     noticeably worse. Zhaoxin processors are an exception, the lowbound is not
+     suitable for them based on actual test data.  */
+  if (!CPU_FEATURE_USABLE_P (cpu_features, ERMS)
+      && cpu_features->basic.kind != arch_kind_zhaoxin)
     non_temporal_threshold = non_temporal_threshold_lowbound;
   /* SIZE_MAX >> 4 because memmove-vec-unaligned-erms right-shifts the value of
      'x86_non_temporal_threshold' by `LOG_4X_MEMCPY_THRESH` (4) and it is best
-- 
2.27.0

