From 0bcb18fc0c90e6e1ad10a457de5765e7ff609be7 Mon Sep 17 00:00:00 2001
From: Junchong Pan <panjunchong@hisilicon.com>
Date: Wed, 2 Mar 2022 07:15:19 +0000
Subject: [PATCH 077/109] rsa: fix interface name and log msg

wd_rsa_key_bits() is used to get key bits,
changing its name to wd_rsa_get_key_bits()
can make the semantics clearer.

Signed-off-by: Junchong Pan <panjunchong@hisilicon.com>
Signed-off-by: Zhiqi Song <songzhiqi1@huawei.com>
---
 include/wd_rsa.h                     | 2 +-
 test/hisi_hpre_test/test_hisi_hpre.c | 6 +++---
 wd_rsa.c                             | 4 ++--
 3 files changed, 6 insertions(+), 6 deletions(-)

diff --git a/include/wd_rsa.h b/include/wd_rsa.h
index 081bc2a..0978b79 100644
--- a/include/wd_rsa.h
+++ b/include/wd_rsa.h
@@ -67,7 +67,7 @@ struct wd_rsa_sess_setup {
 };
 
 bool wd_rsa_is_crt(handle_t sess);
-__u32 wd_rsa_key_bits(handle_t sess);
+__u32 wd_rsa_get_key_bits(handle_t sess);
 void wd_rsa_get_pubkey(handle_t sess, struct wd_rsa_pubkey **pubkey);
 void wd_rsa_get_prikey(handle_t sess, struct wd_rsa_prikey **prikey);
 int wd_rsa_set_pubkey_params(handle_t sess, struct wd_dtb *e, struct wd_dtb *n);
diff --git a/test/hisi_hpre_test/test_hisi_hpre.c b/test/hisi_hpre_test/test_hisi_hpre.c
index 924adb7..57d76fd 100644
--- a/test/hisi_hpre_test/test_hisi_hpre.c
+++ b/test/hisi_hpre_test/test_hisi_hpre.c
@@ -6793,7 +6793,7 @@ static int get_rsa_key_from_test_sample(handle_t sess, char *pubkey_file,
 	memset(&wd_q, 0, sizeof(wd_q));
 	memset(&wd_p, 0, sizeof(wd_p));
 
-	bits = wd_rsa_key_bits(sess);
+	bits = wd_rsa_get_key_bits(sess);
 	if (bits == 1024) {
 		e = rsa_e_1024;
 		p = rsa_p_1024;
@@ -7348,7 +7348,7 @@ int hpre_test_result_check(handle_t sess,  struct wd_rsa_req *req, void *key)
 	}
 
 	wd_rsa_get_prikey(sess, &prikey);
-	keybits = wd_rsa_key_bits(sess);
+	keybits = wd_rsa_get_key_bits(sess);
 	key_size = keybits >> 3;
 	if (req->op_type == WD_RSA_GENKEY) {
 		if (wd_rsa_is_crt(sess)) {
@@ -7907,7 +7907,7 @@ static void _rsa_cb(void *req_t)
 	struct test_hpre_pthread_dt *thread_info = tag->thread_info;
 
 	wd_rsa_get_prikey(sess, &prikey);
-	keybits = wd_rsa_key_bits(sess);
+	keybits = wd_rsa_get_key_bits(sess);
 	key_size = keybits >> 3;
 
 	thread_info->recv_task_num++;
diff --git a/wd_rsa.c b/wd_rsa.c
index 2e61927..4c8fd71 100644
--- a/wd_rsa.c
+++ b/wd_rsa.c
@@ -599,7 +599,7 @@ struct wd_rsa_kg_out *wd_rsa_new_kg_out(handle_t sess)
 
 	kg_out = malloc(kg_out_size + sizeof(*kg_out));
 	if (!kg_out) {
-		WD_ERR("sess malloc kg_in memory fail!\n");
+		WD_ERR("sess malloc kg_out memory fail!\n");
 		return NULL;
 	}
 
@@ -875,7 +875,7 @@ bool wd_rsa_is_crt(handle_t sess)
 	return ((struct wd_rsa_sess *)sess)->setup.is_crt;
 }
 
-__u32 wd_rsa_key_bits(handle_t sess)
+__u32 wd_rsa_get_key_bits(handle_t sess)
 {
 	if (!sess) {
 		WD_ERR("get rsa key bits, sess NULL!\n");
-- 
2.27.0

