From 4e2b91f8079ad1195e20c730cda4e33643918257 Mon Sep 17 00:00:00 2001
From: Kai Ye <yekai13@huawei.com>
Date: Tue, 8 Mar 2022 16:14:17 +0800
Subject: [PATCH 085/109] drv/sec: support sm4-ecb alg by new fs

Kunpeng 920 can supports sm4-ecb by test, and has
been updated the chip fs.

Signed-off-by: Kai Ye <yekai13@huawei.com>
---
 drv/hisi_sec.c         | 4 ----
 v1/drv/hisi_sec_udrv.c | 4 ----
 2 files changed, 8 deletions(-)

diff --git a/drv/hisi_sec.c b/drv/hisi_sec.c
index 264d850..16fcb5f 100644
--- a/drv/hisi_sec.c
+++ b/drv/hisi_sec.c
@@ -656,10 +656,6 @@ static int fill_cipher_bd2_mode(struct wd_cipher_msg *msg,
 
 	switch (msg->mode) {
 	case WD_CIPHER_ECB:
-		if (msg->alg == WD_CIPHER_SM4) {
-			WD_ERR("kunpeng 920 not support ECB(SM4)!\n");
-			return -WD_EINVAL;
-		}
 		c_mode = C_MODE_ECB;
 		break;
 	case WD_CIPHER_CBC:
diff --git a/v1/drv/hisi_sec_udrv.c b/v1/drv/hisi_sec_udrv.c
index 7345baf..3e1e7d1 100644
--- a/v1/drv/hisi_sec_udrv.c
+++ b/v1/drv/hisi_sec_udrv.c
@@ -165,10 +165,6 @@ static int fill_cipher_bd2_mode(struct wcrypto_cipher_msg *msg,
 
 	switch (msg->mode) {
 	case WCRYPTO_CIPHER_ECB:
-		if (msg->alg == WCRYPTO_CIPHER_SM4) {
-			WD_ERR("kunpeng 920 not support ECB(SM4)!\n");
-			return -WD_EINVAL;
-		}
 		sqe->type2.c_mode = C_MODE_ECB;
 		break;
 	case WCRYPTO_CIPHER_CBC:
-- 
2.27.0

