From d554782317fb25319690c2f6453994494a0396d0 Mon Sep 17 00:00:00 2001
From: JunchongPan <panjunchong@hisilicon.com>
Date: Thu, 10 Mar 2022 20:58:46 +0800
Subject: [PATCH 087/109] uadk/qm_udrv: Modify goto err_out

In setup_region, when mmap_qfr return NULL, don't need
to set sq_base/mmio_base NULL, return ENOMEM direct.

Signed-off-by: JunchongPan <panjunchong@hisilicon.com>
---
 drv/hisi_qm_udrv.c | 9 ++-------
 1 file changed, 2 insertions(+), 7 deletions(-)

diff --git a/drv/hisi_qm_udrv.c b/drv/hisi_qm_udrv.c
index 2e692a1..906dfa3 100644
--- a/drv/hisi_qm_udrv.c
+++ b/drv/hisi_qm_udrv.c
@@ -168,22 +168,17 @@ static int hisi_qm_setup_region(handle_t h_ctx,
 	q_info->sq_base = wd_ctx_mmap_qfr(h_ctx, UACCE_QFRT_DUS);
 	if (!q_info->sq_base) {
 		WD_ERR("mmap dus fail\n");
-		goto err_out;
+		return -WD_ENOMEM;
 	}
 
 	q_info->mmio_base = wd_ctx_mmap_qfr(h_ctx, UACCE_QFRT_MMIO);
 	if (!q_info->mmio_base) {
 		wd_ctx_unmap_qfr(h_ctx, UACCE_QFRT_DUS);
 		WD_ERR("mmap mmio fail\n");
-		goto err_out;
+		return -WD_ENOMEM;
 	}
 
 	return 0;
-
-err_out:
-	q_info->sq_base = NULL;
-	q_info->mmio_base = NULL;
-	return -WD_ENOMEM;
 }
 
 static void hisi_qm_unset_region(handle_t h_ctx,
-- 
2.27.0

