From f2d35154e52052e315a193900157dc9a0e2f3fb9 Mon Sep 17 00:00:00 2001
From: Yunhui Cui <cuiyunhui@bytedance.com>
Date: Mon, 19 Feb 2024 17:34:17 +0800
Subject: [PATCH] lscpu: add RISC-V CPUTYPE support

Only after adding cpu type can print the remaining cpu information,
such as cacheinfo.

Signed-off-by: Yunhui Cui <cuiyunhui@bytedance.com>
Signed-off-by: yuanchicheng <chicheng.oerv@isrc.iscas.ac.cn>
---
 sys-utils/lscpu-cputype.c | 1 +
 1 file changed, 1 insertion(+)

diff --git a/sys-utils/lscpu-cputype.c b/sys-utils/lscpu-cputype.c
index bcdf06e8db0..4ca3d353299 100644
--- a/sys-utils/lscpu-cputype.c
+++ b/sys-utils/lscpu-cputype.c
@@ -212,6 +212,7 @@
 	DEF_PAT_CPUTYPE( "family",		PAT_FAMILY,	family),
 	DEF_PAT_CPUTYPE( "features",		PAT_FEATURES,	flags),		/* s390 */
 	DEF_PAT_CPUTYPE( "flags",		PAT_FLAGS,	flags),		/* x86 */
+	DEF_PAT_CPUTYPE( "hart isa",            PAT_ISA,        isa),           /* riscv */
 	DEF_PAT_CPUTYPE( "max thread id",	PAT_MAX_THREAD_ID, mtid),	/* s390 */
 	DEF_PAT_CPUTYPE( "model",		PAT_MODEL,	model),
 	DEF_PAT_CPUTYPE( "model name",		PAT_MODEL_NAME,	modelname),
