From d5eb70924f87963c80c7a4677048f2bcd4581534 Mon Sep 17 00:00:00 2001
From: zhoupengcheng <zhoupengcheng11@huawei.com>
Date: Mon, 18 Mar 2024 20:44:27 +0800
Subject: [PATCH] adapt sqlite 3.42 to resolve the build failure.

---
 database/init.sql | 562 +++++++++++++++++++++++-----------------------
 1 file changed, 281 insertions(+), 281 deletions(-)

diff --git a/database/init.sql b/database/init.sql
index b8edb3a..688743c 100755
--- a/database/init.sql
+++ b/database/init.sql
@@ -77,305 +77,305 @@ CREATE TABLE IF NOT EXISTS schedule(
 
 
 -- class_apps:
-INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES("encryption_AES", "encryption", "", 0);
-INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES("encryption_MD5", "encryption", "", 0);
-INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES("encryption_RSAPublic", "encryption", "", 0);
-INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES("default", "default", "", 0);
-INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES("ceph", "storage-ceph", "", 0);
-INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES("hadoop_hdd", "big-data-hadoop-hdfs", "", 0);
-INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES("hadoop_ssd", "big-data-hadoop-hdfs", "", 0);
-INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES("spark", "big-data-hadoop-spark", "", 0);
-INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES("mongodb", "database-mongodb", "", 0);
-INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES("mariadb", "database-mariadb", "", 0);
-INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES("mysql", "database-mysql", "", 0);
-INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES("postgresql", "database-postgresql", "", 0);
-INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES("nginx_https_long", "web-nginx", "", 0);
-INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES("nginx_https_short", "web-nginx", "", 0);
-INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES("nginx_http_long", "web-nginx", "", 0);
-INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES("nginx_http_short", "web-nginx", "", 0);
-INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES("apache", "web-apache-traffic-server", "", 0);
-INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES("redis", "in-memory-database-redis", "", 0);
-INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES("speccpu", "basic-test-suite-speccpu", "", 0);
-INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES("specjbb", "basic-test-suite-specjbb", "", 0);
-INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES("dubbo", "middleware-dubbo", "", 0);
-INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES("robox", "arm-native-android-container", "", 0);
-INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES("kvm", "cloud-compute-kvm", "", 0);
-INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES("hpc", "hpc-gatk4", "", 0);
-INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES("olc", "virtualization-consumer-cloud", "", 0);
-INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES("mariadb_kvm", "virtualization-mariadb", "", 0);
-INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES("mariadb_docker", "docker-mariadb", "", 0);
+INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES('encryption_AES', 'encryption', '', 0);
+INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES('encryption_MD5', 'encryption', '', 0);
+INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES('encryption_RSAPublic', 'encryption', '', 0);
+INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES('default', 'default', '', 0);
+INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES('ceph', 'storage-ceph', '', 0);
+INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES('hadoop_hdd', 'big-data-hadoop-hdfs', '', 0);
+INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES('hadoop_ssd', 'big-data-hadoop-hdfs', '', 0);
+INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES('spark', 'big-data-hadoop-spark', '', 0);
+INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES('mongodb', 'database-mongodb', '', 0);
+INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES('mariadb', 'database-mariadb', '', 0);
+INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES('mysql', 'database-mysql', '', 0);
+INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES('postgresql', 'database-postgresql', '', 0);
+INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES('nginx_https_long', 'web-nginx', '', 0);
+INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES('nginx_https_short', 'web-nginx', '', 0);
+INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES('nginx_http_long', 'web-nginx', '', 0);
+INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES('nginx_http_short', 'web-nginx', '', 0);
+INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES('apache', 'web-apache-traffic-server', '', 0);
+INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES('redis', 'in-memory-database-redis', '', 0);
+INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES('speccpu', 'basic-test-suite-speccpu', '', 0);
+INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES('specjbb', 'basic-test-suite-specjbb', '', 0);
+INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES('dubbo', 'middleware-dubbo', '', 0);
+INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES('robox', 'arm-native-android-container', '', 0);
+INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES('kvm', 'cloud-compute-kvm', '', 0);
+INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES('hpc', 'hpc-gatk4', '', 0);
+INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES('olc', 'virtualization-consumer-cloud', '', 0);
+INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES('mariadb_kvm', 'virtualization-mariadb', '', 0);
+INSERT INTO class_apps(class, apps, resource_limit, deletable) VALUES('mariadb_docker', 'docker-mariadb', '', 0);
 
 -- class_profile:
-INSERT INTO class_profile(class, profile_type, active) VALUES("encryption_AES", "encryption-AES-chauffeur", 0);
-INSERT INTO class_profile(class, profile_type, active) VALUES("encryption_MD5", "encryption-MD5-chauffeur", 0);
-INSERT INTO class_profile(class, profile_type, active) VALUES("encryption_RSAPublic", "encryption-RSAPublic-chauffeur", 0);
-INSERT INTO class_profile(class, profile_type, active) VALUES("default", "default-default", 0);
-INSERT INTO class_profile(class, profile_type, active) VALUES("ceph", "storage-ceph-vdbench-hdd", 0);
-INSERT INTO class_profile(class, profile_type, active) VALUES("hadoop_hdd", "big-data-hadoop-hdfs-dfsio-hdd", 0);
-INSERT INTO class_profile(class, profile_type, active) VALUES("hadoop_ssd", "big-data-hadoop-hdfs-dfsio-ssd", 0);
-INSERT INTO class_profile(class, profile_type, active) VALUES("spark", "big-data-hadoop-spark-kmeans", 0);
-INSERT INTO class_profile(class, profile_type, active) VALUES("mongodb", "database-mongodb-2p-sysbench", 0);
-INSERT INTO class_profile(class, profile_type, active) VALUES("mariadb", "database-mariadb-2p-tpcc-c3", 0);
-INSERT INTO class_profile(class, profile_type, active) VALUES("mysql", "database-mysql-2p-sysbench-hdd", 0);
-INSERT INTO class_profile(class, profile_type, active) VALUES("postgresql", "database-postgresql-2p-sysbench-hdd", 0);
-INSERT INTO class_profile(class, profile_type, active) VALUES("nginx_https_short", "web-nginx-https-short-connection", 0);
-INSERT INTO class_profile(class, profile_type, active) VALUES("nginx_https_long", "web-nginx-https-long-connection", 0);
-INSERT INTO class_profile(class, profile_type, active) VALUES("nginx_http_short", "web-nginx-http-short-connection", 0);
-INSERT INTO class_profile(class, profile_type, active) VALUES("nginx_http_long", "web-nginx-http-long-connection", 0);
-INSERT INTO class_profile(class, profile_type, active) VALUES("apache", "web-apache-traffic-server-spirent-pingpo", 0);
-INSERT INTO class_profile(class, profile_type, active) VALUES("redis", "in-memory-database-redis-redis-benchmark", 0);
-INSERT INTO class_profile(class, profile_type, active) VALUES("speccpu", "basic-test-suite-speccpu-speccpu2006", 0);
-INSERT INTO class_profile(class, profile_type, active) VALUES("specjbb", "basic-test-suite-specjbb-specjbb2015", 0);
-INSERT INTO class_profile(class, profile_type, active) VALUES("dubbo", "middleware-dubbo-dubbo-benchmark", 0);
-INSERT INTO class_profile(class, profile_type, active) VALUES("robox", "arm-native-android-container-robox", 0);
-INSERT INTO class_profile(class, profile_type, active) VALUES("kvm", "cloud-compute-kvm-host", 0);
-INSERT INTO class_profile(class, profile_type, active) VALUES("hpc", "hpc-gatk4-human-genome", 0);
-INSERT INTO class_profile(class, profile_type, active) VALUES("olc", "virtualization-consumer-cloud-olc", 0);
-INSERT INTO class_profile(class, profile_type, active) VALUES("mariadb_kvm", "virtualization-mariadb-2p-tpcc-c3", 0);
-INSERT INTO class_profile(class, profile_type, active) VALUES("mariadb_docker", "docker-mariadb-2p-tpcc-c3", 0);
+INSERT INTO class_profile(class, profile_type, active) VALUES('encryption_AES', 'encryption-AES-chauffeur', 0);
+INSERT INTO class_profile(class, profile_type, active) VALUES('encryption_MD5', 'encryption-MD5-chauffeur', 0);
+INSERT INTO class_profile(class, profile_type, active) VALUES('encryption_RSAPublic', 'encryption-RSAPublic-chauffeur', 0);
+INSERT INTO class_profile(class, profile_type, active) VALUES('default', 'default-default', 0);
+INSERT INTO class_profile(class, profile_type, active) VALUES('ceph', 'storage-ceph-vdbench-hdd', 0);
+INSERT INTO class_profile(class, profile_type, active) VALUES('hadoop_hdd', 'big-data-hadoop-hdfs-dfsio-hdd', 0);
+INSERT INTO class_profile(class, profile_type, active) VALUES('hadoop_ssd', 'big-data-hadoop-hdfs-dfsio-ssd', 0);
+INSERT INTO class_profile(class, profile_type, active) VALUES('spark', 'big-data-hadoop-spark-kmeans', 0);
+INSERT INTO class_profile(class, profile_type, active) VALUES('mongodb', 'database-mongodb-2p-sysbench', 0);
+INSERT INTO class_profile(class, profile_type, active) VALUES('mariadb', 'database-mariadb-2p-tpcc-c3', 0);
+INSERT INTO class_profile(class, profile_type, active) VALUES('mysql', 'database-mysql-2p-sysbench-hdd', 0);
+INSERT INTO class_profile(class, profile_type, active) VALUES('postgresql', 'database-postgresql-2p-sysbench-hdd', 0);
+INSERT INTO class_profile(class, profile_type, active) VALUES('nginx_https_short', 'web-nginx-https-short-connection', 0);
+INSERT INTO class_profile(class, profile_type, active) VALUES('nginx_https_long', 'web-nginx-https-long-connection', 0);
+INSERT INTO class_profile(class, profile_type, active) VALUES('nginx_http_short', 'web-nginx-http-short-connection', 0);
+INSERT INTO class_profile(class, profile_type, active) VALUES('nginx_http_long', 'web-nginx-http-long-connection', 0);
+INSERT INTO class_profile(class, profile_type, active) VALUES('apache', 'web-apache-traffic-server-spirent-pingpo', 0);
+INSERT INTO class_profile(class, profile_type, active) VALUES('redis', 'in-memory-database-redis-redis-benchmark', 0);
+INSERT INTO class_profile(class, profile_type, active) VALUES('speccpu', 'basic-test-suite-speccpu-speccpu2006', 0);
+INSERT INTO class_profile(class, profile_type, active) VALUES('specjbb', 'basic-test-suite-specjbb-specjbb2015', 0);
+INSERT INTO class_profile(class, profile_type, active) VALUES('dubbo', 'middleware-dubbo-dubbo-benchmark', 0);
+INSERT INTO class_profile(class, profile_type, active) VALUES('robox', 'arm-native-android-container-robox', 0);
+INSERT INTO class_profile(class, profile_type, active) VALUES('kvm', 'cloud-compute-kvm-host', 0);
+INSERT INTO class_profile(class, profile_type, active) VALUES('hpc', 'hpc-gatk4-human-genome', 0);
+INSERT INTO class_profile(class, profile_type, active) VALUES('olc', 'virtualization-consumer-cloud-olc', 0);
+INSERT INTO class_profile(class, profile_type, active) VALUES('mariadb_kvm', 'virtualization-mariadb-2p-tpcc-c3', 0);
+INSERT INTO class_profile(class, profile_type, active) VALUES('mariadb_docker', 'docker-mariadb-2p-tpcc-c3', 0);
 
 -- Performance Point
-INSERT INTO tuned_item(property, item) VALUES("check_environment", "Check");
+INSERT INTO tuned_item(property, item) VALUES('check_environment', 'Check');
 
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_HZ", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_ARM64_64K_PAGES", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_NUMA_AWARE_SPINLOCKS", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_CGROUP_FILES", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_SLUB_DEBUG", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_PM_DEBUG", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_PM_SLEEP_DEBUG", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_STACKPROTECTOR", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_STACKPROTECTOR_STRONG", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_VMAP_STACK", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_BLK_DEBUG_FS", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_BLK_DEBUG_FS_ZONED", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_NET_DROP_MONITOR", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_DM_DEBUG", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_MLX4_DEBUG", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_VIDEO_ADV_DEBUG", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_INFINIBAND_IPOIB_DEBUG", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_NFS_DEBUG", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_SUNRPC_DEBUG", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_CIFS_DEBUG", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_BINARY_PRINTF", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_DEBUG_INFO_DWARF4", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_DEBUG_MEMORY_INIT", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_SCHED_DEBUG", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_DEBUG_BUGVERBOSE", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_DEBUG_LIST", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_TRACEPOINTS", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_NOP_TRACER", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_TRACER_MAX_TRACE", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_TRACE_CLOCK", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_RING_BUFFER", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_EVENT_TRACING", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_CONTEXT_SWITCH_TRACER", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_TRACING", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_GENERIC_TRACER", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_FTRACE", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_FUNCTION_TRACER", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_FUNCTION_GRAPH_TRACER", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_SCHED_TRACER", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_HWLAT_TRACER", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_FTRACE_SYSCALLS", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_TRACER_SNAPSHOT", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_BRANCH_PROFILE_NONE", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_STACK_TRACER", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_BLK_DEV_IO_TRACE", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_KPROBE_EVENTS", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_UPROBE_EVENTS", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_BPF_EVENTS", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_PROBE_EVENTS", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_DYNAMIC_FTRACE", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_FTRACE_MCOUNT_RECORD", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_TRACING_MAP", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_HIST_TRIGGERS", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_RING_BUFFER_BENCHMARK", "Kernel");
-INSERT INTO tuned_item(property, item) VALUES("CONFIG_DEBUG_ALIGN_RODATA", "Kernel");
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_HZ', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_ARM64_64K_PAGES', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_NUMA_AWARE_SPINLOCKS', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_CGROUP_FILES', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_SLUB_DEBUG', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_PM_DEBUG', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_PM_SLEEP_DEBUG', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_STACKPROTECTOR', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_STACKPROTECTOR_STRONG', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_VMAP_STACK', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_BLK_DEBUG_FS', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_BLK_DEBUG_FS_ZONED', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_NET_DROP_MONITOR', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_DM_DEBUG', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_MLX4_DEBUG', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_VIDEO_ADV_DEBUG', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_INFINIBAND_IPOIB_DEBUG', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_NFS_DEBUG', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_SUNRPC_DEBUG', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_CIFS_DEBUG', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_BINARY_PRINTF', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_DEBUG_INFO_DWARF4', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_DEBUG_MEMORY_INIT', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_SCHED_DEBUG', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_DEBUG_BUGVERBOSE', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_DEBUG_LIST', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_TRACEPOINTS', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_NOP_TRACER', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_TRACER_MAX_TRACE', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_TRACE_CLOCK', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_RING_BUFFER', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_EVENT_TRACING', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_CONTEXT_SWITCH_TRACER', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_TRACING', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_GENERIC_TRACER', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_FTRACE', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_FUNCTION_TRACER', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_FUNCTION_GRAPH_TRACER', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_SCHED_TRACER', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_HWLAT_TRACER', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_FTRACE_SYSCALLS', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_TRACER_SNAPSHOT', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_BRANCH_PROFILE_NONE', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_STACK_TRACER', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_BLK_DEV_IO_TRACE', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_KPROBE_EVENTS', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_UPROBE_EVENTS', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_BPF_EVENTS', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_PROBE_EVENTS', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_DYNAMIC_FTRACE', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_FTRACE_MCOUNT_RECORD', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_TRACING_MAP', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_HIST_TRIGGERS', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_RING_BUFFER_BENCHMARK', 'Kernel');
+INSERT INTO tuned_item(property, item) VALUES('CONFIG_DEBUG_ALIGN_RODATA', 'Kernel');
 
-INSERT INTO tuned_item(property, item) VALUES("iommu.passthrough", "Bootloader");
-INSERT INTO tuned_item(property, item) VALUES("iommu.strict", "Bootloader");
-INSERT INTO tuned_item(property, item) VALUES("default_hugepagesz", "Bootloader");
-INSERT INTO tuned_item(property, item) VALUES("hugepagesz", "Bootloader");
-INSERT INTO tuned_item(property, item) VALUES("hugepages", "Bootloader");
-INSERT INTO tuned_item(property, item) VALUES("selinux", "Bootloader");
-INSERT INTO tuned_item(property, item) VALUES("skew_tick", "Bootloader");
-INSERT INTO tuned_item(property, item) VALUES("numa_spinlock", "Bootloader");
-INSERT INTO tuned_item(property, item) VALUES("scsi_mod.use_blk_mq", "Bootloader");
-INSERT INTO tuned_item(property, item) VALUES("sched_steal_node_limit", "Bootloader");
+INSERT INTO tuned_item(property, item) VALUES('iommu.passthrough', 'Bootloader');
+INSERT INTO tuned_item(property, item) VALUES('iommu.strict', 'Bootloader');
+INSERT INTO tuned_item(property, item) VALUES('default_hugepagesz', 'Bootloader');
+INSERT INTO tuned_item(property, item) VALUES('hugepagesz', 'Bootloader');
+INSERT INTO tuned_item(property, item) VALUES('hugepages', 'Bootloader');
+INSERT INTO tuned_item(property, item) VALUES('selinux', 'Bootloader');
+INSERT INTO tuned_item(property, item) VALUES('skew_tick', 'Bootloader');
+INSERT INTO tuned_item(property, item) VALUES('numa_spinlock', 'Bootloader');
+INSERT INTO tuned_item(property, item) VALUES('scsi_mod.use_blk_mq', 'Bootloader');
+INSERT INTO tuned_item(property, item) VALUES('sched_steal_node_limit', 'Bootloader');
 
-INSERT INTO tuned_item(property, item) VALUES("openssl_hpre", "Script");
-INSERT INTO tuned_item(property, item) VALUES("hinic", "Script");
+INSERT INTO tuned_item(property, item) VALUES('openssl_hpre', 'Script');
+INSERT INTO tuned_item(property, item) VALUES('hinic', 'Script');
 
-INSERT INTO tuned_item(property, item) VALUES("NUMA", "Bios");
-INSERT INTO tuned_item(property, item) VALUES("SRIOV", "Bios");
-INSERT INTO tuned_item(property, item) VALUES("Custom Refresh Rate", "Bios");
-INSERT INTO tuned_item(property, item) VALUES("Stream Write Mode", "Bios");
-INSERT INTO tuned_item(property, item) VALUES("Support Smmu", "Bios");
-INSERT INTO tuned_item(property, item) VALUES("Support SPCR", "Bios");
-INSERT INTO tuned_item(property, item) VALUES("Max Payload Size", "Bios");
-INSERT INTO tuned_item(property, item) VALUES("Power Policy", "Bios");
-INSERT INTO tuned_item(property, item) VALUES("Rank Interleaving", "Bios");
-INSERT INTO tuned_item(property, item) VALUES("Read Policy", "Bios");
-INSERT INTO tuned_item(property, item) VALUES("Write Policy", "Bios");
-INSERT INTO tuned_item(property, item) VALUES("I/O Policy", "Bios");
-INSERT INTO tuned_item(property, item) VALUES("Access Policy", "Bios");
-INSERT INTO tuned_item(property, item) VALUES("Drive Cache", "Bios");
+INSERT INTO tuned_item(property, item) VALUES('NUMA', 'Bios');
+INSERT INTO tuned_item(property, item) VALUES('SRIOV', 'Bios');
+INSERT INTO tuned_item(property, item) VALUES('Custom Refresh Rate', 'Bios');
+INSERT INTO tuned_item(property, item) VALUES('Stream Write Mode', 'Bios');
+INSERT INTO tuned_item(property, item) VALUES('Support Smmu', 'Bios');
+INSERT INTO tuned_item(property, item) VALUES('Support SPCR', 'Bios');
+INSERT INTO tuned_item(property, item) VALUES('Max Payload Size', 'Bios');
+INSERT INTO tuned_item(property, item) VALUES('Power Policy', 'Bios');
+INSERT INTO tuned_item(property, item) VALUES('Rank Interleaving', 'Bios');
+INSERT INTO tuned_item(property, item) VALUES('Read Policy', 'Bios');
+INSERT INTO tuned_item(property, item) VALUES('Write Policy', 'Bios');
+INSERT INTO tuned_item(property, item) VALUES('I/O Policy', 'Bios');
+INSERT INTO tuned_item(property, item) VALUES('Access Policy', 'Bios');
+INSERT INTO tuned_item(property, item) VALUES('Drive Cache', 'Bios');
 
-INSERT INTO tuned_item(property, item) VALUES("vm.nr_hugepages", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("vm.swappiness", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("vm.dirty_ratio", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("vm.max_map_count", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("vm.panic_on_oom", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("vm.dirty_background_ratio", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("vm.dirty_writeback_centisecs", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("vm.dirty_expire_centisecs", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("vm.overcommit_memory", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("vm.zone_reclaim_mode", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("vm.min_free_kbytes", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("kernel/mm/transparent_hugepage/defrag", "Sysfs");
-INSERT INTO tuned_item(property, item) VALUES("kernel/mm/transparent_hugepage/enabled", "Sysfs");
-INSERT INTO tuned_item(property, item) VALUES("kernel/debug/sched_features", "Sysfs");
-INSERT INTO tuned_item(property, item) VALUES("block/{disk}/queue/scheduler", "Sysfs");
-INSERT INTO tuned_item(property, item) VALUES("block/{disk}/queue/read_ahead_kb", "Sysfs");
-INSERT INTO tuned_item(property, item) VALUES("block/{disk}/queue/nr_requests", "Sysfs");
-INSERT INTO tuned_item(property, item) VALUES("block/{disk}/device/queue_depth", "Sysfs");
-INSERT INTO tuned_item(property, item) VALUES("block/{disk}/queue/write_cache", "Sysfs");
-INSERT INTO tuned_item(property, item) VALUES("block/{disk}/queue/nomerges", "Sysfs");
-INSERT INTO tuned_item(property, item) VALUES("block/{disk}/queue/iosched/slice_idle", "Sysfs");
-INSERT INTO tuned_item(property, item) VALUES("block/{disk}/queue/iosched/low_latency", "Sysfs");
-INSERT INTO tuned_item(property, item) VALUES("block/{disk}/queue/rq_affinity", "Sysfs");
-INSERT INTO tuned_item(property, item) VALUES("block/{disk}/queue/max_sectors_kb", "Sysfs");
-INSERT INTO tuned_item(property, item) VALUES("net.ipv4.tcp_max_syn_backlog", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.core.somaxconn", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.ipv4.tcp_keepalive_time", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.ipv4.tcp_keepalive_probes", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.ipv4.tcp_keepalive_intvl", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.ipv4.tcp_retries2", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.ipv4.ip_forward", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.ipv4.conf.default.rp_filter", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.ipv4.conf.default.accept_source_route", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.ipv4.tcp_tw_reuse", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.ipv4.tcp_syncookies", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.ipv4.tcp_low_latency", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.netfilter.nf_conntrack_max", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.netfilter.nf_conntrack_tcp_timeout_established", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.bridge.bridge-nf-call-ip6tables", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.bridge.bridge-nf-call-iptables", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.bridge.bridge-nf-call-arptables", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.ipv4.ip_local_port_range", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.ipv4.tcp_max_tw_buckets", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.core.netdev_max_backlog", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.ipv4.tcp_max_orphans", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.ipv4.tcp_timestamps", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.ipv4.tcp_synack_retries", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.ipv4.tcp_syn_retries", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.ipv4.tcp_fin_timeout", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.ipv4.tcp_mem", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.ipv4.tcp_rmem", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.ipv4.tcp_wmem", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.ipv4.udp_mem", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.ipv4.tcp_sack", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.ipv4.tcp_fastopen", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.core.wmem_default", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.core.rmem_default", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.core.rmem_max", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.core.wmem_max", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.netfilter.nf_conntrack_tcp_timeout_close_wait", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.netfilter.nf_conntrack_tcp_timeout_fin_wait", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.netfilter.nf_conntrack_tcp_timeout_time_wait", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.ipv4.conf.default.forwarding", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.netfilter.nf_conntrack_buckets", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.netfilter.nf_conntrack_count", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.nf_conntrack_max", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.core.dev_weight", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.core.optmem_max", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.core.netdev_budget", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.core.busy_read", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.core.busy_poll", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("net.core.rps_sock_flow_entries", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("ethtool", "Script");
-INSERT INTO tuned_item(property, item) VALUES("ifconfig", "Script");
-INSERT INTO tuned_item(property, item) VALUES("fs.file-max", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("fs.nr_open", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("fs.suid_dumpable", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("fs.aio-max-nr", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("fs.inotify.max_user_instances", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("kernel.threads-max", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("kernel.sem", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("kernel.msgmnb", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("kernel.msgmax", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("kernel.shmmax", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("kernel.shmall", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("kernel.shmmni", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("kernel.pid_max", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("kernel.numa_balancing", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("{user}.hard.nofile", "Ulimit");
-INSERT INTO tuned_item(property, item) VALUES("{user}.soft.nofile", "Ulimit");
-INSERT INTO tuned_item(property, item) VALUES("{user}.soft.stack", "Ulimit");
-INSERT INTO tuned_item(property, item) VALUES("{user}.hard.stack", "Ulimit");
-INSERT INTO tuned_item(property, item) VALUES("{user}.soft.nproc", "Ulimit");
-INSERT INTO tuned_item(property, item) VALUES("{user}.hard.nproc", "Ulimit");
-INSERT INTO tuned_item(property, item) VALUES("{user}.soft.memlock", "Ulimit");
-INSERT INTO tuned_item(property, item) VALUES("{user}.hard.memlock", "Ulimit");
-INSERT INTO tuned_item(property, item) VALUES("swap", "Script");
-INSERT INTO tuned_item(property, item) VALUES("kernel.randomize_va_space", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("kernel.sched_cfs_bandwidth_slice_us", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("kernel.sched_migration_cost_ns", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("kernel.sched_latency_ns", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("kernel.sched_nr_migrate", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("kernel.sched_min_granularity_ns", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("kernel.sched_wakeup_granularity_ns", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("kernel.sysrq", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("kernel.kstack_depth_to_print", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("kernel.panic_on_oops", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("kernel.panic", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("kernel.hung_task_timeout_secs", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("kernel.hung_task_panic", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("vm.oom_dump_tasks", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("kernel.softlockup_panic", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("kernel.core_uses_pid", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("kernel.nmi_watchdog", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("kernel.sched_rt_runtime_us", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("vm.stat_interval", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("kernel.timer_migration", "Sysctl");
-INSERT INTO tuned_item(property, item) VALUES("kernel.sched_autogroup_enabled", "Sysctl");
+INSERT INTO tuned_item(property, item) VALUES('vm.nr_hugepages', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('vm.swappiness', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('vm.dirty_ratio', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('vm.max_map_count', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('vm.panic_on_oom', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('vm.dirty_background_ratio', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('vm.dirty_writeback_centisecs', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('vm.dirty_expire_centisecs', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('vm.overcommit_memory', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('vm.zone_reclaim_mode', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('vm.min_free_kbytes', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('kernel/mm/transparent_hugepage/defrag', 'Sysfs');
+INSERT INTO tuned_item(property, item) VALUES('kernel/mm/transparent_hugepage/enabled', 'Sysfs');
+INSERT INTO tuned_item(property, item) VALUES('kernel/debug/sched_features', 'Sysfs');
+INSERT INTO tuned_item(property, item) VALUES('block/{disk}/queue/scheduler', 'Sysfs');
+INSERT INTO tuned_item(property, item) VALUES('block/{disk}/queue/read_ahead_kb', 'Sysfs');
+INSERT INTO tuned_item(property, item) VALUES('block/{disk}/queue/nr_requests', 'Sysfs');
+INSERT INTO tuned_item(property, item) VALUES('block/{disk}/device/queue_depth', 'Sysfs');
+INSERT INTO tuned_item(property, item) VALUES('block/{disk}/queue/write_cache', 'Sysfs');
+INSERT INTO tuned_item(property, item) VALUES('block/{disk}/queue/nomerges', 'Sysfs');
+INSERT INTO tuned_item(property, item) VALUES('block/{disk}/queue/iosched/slice_idle', 'Sysfs');
+INSERT INTO tuned_item(property, item) VALUES('block/{disk}/queue/iosched/low_latency', 'Sysfs');
+INSERT INTO tuned_item(property, item) VALUES('block/{disk}/queue/rq_affinity', 'Sysfs');
+INSERT INTO tuned_item(property, item) VALUES('block/{disk}/queue/max_sectors_kb', 'Sysfs');
+INSERT INTO tuned_item(property, item) VALUES('net.ipv4.tcp_max_syn_backlog', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.core.somaxconn', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.ipv4.tcp_keepalive_time', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.ipv4.tcp_keepalive_probes', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.ipv4.tcp_keepalive_intvl', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.ipv4.tcp_retries2', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.ipv4.ip_forward', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.ipv4.conf.default.rp_filter', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.ipv4.conf.default.accept_source_route', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.ipv4.tcp_tw_reuse', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.ipv4.tcp_syncookies', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.ipv4.tcp_low_latency', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.netfilter.nf_conntrack_max', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.netfilter.nf_conntrack_tcp_timeout_established', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.bridge.bridge-nf-call-ip6tables', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.bridge.bridge-nf-call-iptables', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.bridge.bridge-nf-call-arptables', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.ipv4.ip_local_port_range', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.ipv4.tcp_max_tw_buckets', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.core.netdev_max_backlog', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.ipv4.tcp_max_orphans', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.ipv4.tcp_timestamps', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.ipv4.tcp_synack_retries', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.ipv4.tcp_syn_retries', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.ipv4.tcp_fin_timeout', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.ipv4.tcp_mem', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.ipv4.tcp_rmem', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.ipv4.tcp_wmem', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.ipv4.udp_mem', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.ipv4.tcp_sack', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.ipv4.tcp_fastopen', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.core.wmem_default', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.core.rmem_default', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.core.rmem_max', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.core.wmem_max', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.netfilter.nf_conntrack_tcp_timeout_close_wait', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.netfilter.nf_conntrack_tcp_timeout_fin_wait', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.netfilter.nf_conntrack_tcp_timeout_time_wait', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.ipv4.conf.default.forwarding', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.netfilter.nf_conntrack_buckets', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.netfilter.nf_conntrack_count', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.nf_conntrack_max', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.core.dev_weight', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.core.optmem_max', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.core.netdev_budget', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.core.busy_read', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.core.busy_poll', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('net.core.rps_sock_flow_entries', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('ethtool', 'Script');
+INSERT INTO tuned_item(property, item) VALUES('ifconfig', 'Script');
+INSERT INTO tuned_item(property, item) VALUES('fs.file-max', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('fs.nr_open', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('fs.suid_dumpable', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('fs.aio-max-nr', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('fs.inotify.max_user_instances', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('kernel.threads-max', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('kernel.sem', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('kernel.msgmnb', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('kernel.msgmax', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('kernel.shmmax', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('kernel.shmall', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('kernel.shmmni', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('kernel.pid_max', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('kernel.numa_balancing', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('{user}.hard.nofile', 'Ulimit');
+INSERT INTO tuned_item(property, item) VALUES('{user}.soft.nofile', 'Ulimit');
+INSERT INTO tuned_item(property, item) VALUES('{user}.soft.stack', 'Ulimit');
+INSERT INTO tuned_item(property, item) VALUES('{user}.hard.stack', 'Ulimit');
+INSERT INTO tuned_item(property, item) VALUES('{user}.soft.nproc', 'Ulimit');
+INSERT INTO tuned_item(property, item) VALUES('{user}.hard.nproc', 'Ulimit');
+INSERT INTO tuned_item(property, item) VALUES('{user}.soft.memlock', 'Ulimit');
+INSERT INTO tuned_item(property, item) VALUES('{user}.hard.memlock', 'Ulimit');
+INSERT INTO tuned_item(property, item) VALUES('swap', 'Script');
+INSERT INTO tuned_item(property, item) VALUES('kernel.randomize_va_space', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('kernel.sched_cfs_bandwidth_slice_us', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('kernel.sched_migration_cost_ns', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('kernel.sched_latency_ns', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('kernel.sched_nr_migrate', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('kernel.sched_min_granularity_ns', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('kernel.sched_wakeup_granularity_ns', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('kernel.sysrq', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('kernel.kstack_depth_to_print', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('kernel.panic_on_oops', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('kernel.panic', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('kernel.hung_task_timeout_secs', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('kernel.hung_task_panic', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('vm.oom_dump_tasks', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('kernel.softlockup_panic', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('kernel.core_uses_pid', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('kernel.nmi_watchdog', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('kernel.sched_rt_runtime_us', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('vm.stat_interval', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('kernel.timer_migration', 'Sysctl');
+INSERT INTO tuned_item(property, item) VALUES('kernel.sched_autogroup_enabled', 'Sysctl');
 
-INSERT INTO tuned_item(property, item) VALUES("prefetch", "Script");
-INSERT INTO tuned_item(property, item) VALUES("logind", "Script");
-INSERT INTO tuned_item(property, item) VALUES("blockdev", "Script");
-INSERT INTO tuned_item(property, item) VALUES("hugepage", "Script");
-INSERT INTO tuned_item(property, item) VALUES("rps_cpus", "Script");
-INSERT INTO tuned_item(property, item) VALUES("sched_domain", "Script");
-INSERT INTO tuned_item(property, item) VALUES("hdparm", "Script");
+INSERT INTO tuned_item(property, item) VALUES('prefetch', 'Script');
+INSERT INTO tuned_item(property, item) VALUES('logind', 'Script');
+INSERT INTO tuned_item(property, item) VALUES('blockdev', 'Script');
+INSERT INTO tuned_item(property, item) VALUES('hugepage', 'Script');
+INSERT INTO tuned_item(property, item) VALUES('rps_cpus', 'Script');
+INSERT INTO tuned_item(property, item) VALUES('sched_domain', 'Script');
+INSERT INTO tuned_item(property, item) VALUES('hdparm', 'Script');
 
-INSERT INTO tuned_item(property, item) VALUES("sysmonitor", "Systemctl");
-INSERT INTO tuned_item(property, item) VALUES("irqbalance", "Systemctl");
-INSERT INTO tuned_item(property, item) VALUES("firewalld", "Systemctl");
-INSERT INTO tuned_item(property, item) VALUES("tuned", "Systemctl");
+INSERT INTO tuned_item(property, item) VALUES('sysmonitor', 'Systemctl');
+INSERT INTO tuned_item(property, item) VALUES('irqbalance', 'Systemctl');
+INSERT INTO tuned_item(property, item) VALUES('firewalld', 'Systemctl');
+INSERT INTO tuned_item(property, item) VALUES('tuned', 'Systemctl');
 
-INSERT INTO tuned_item(property, item) VALUES("compile_optimization", "Compiler");
-INSERT INTO tuned_item(property, item) VALUES("compile_security", "Compiler");
+INSERT INTO tuned_item(property, item) VALUES('compile_optimization', 'Compiler');
+INSERT INTO tuned_item(property, item) VALUES('compile_security', 'Compiler');
 
-INSERT INTO tuned_item(property, item) VALUES("/etc/profile", "Profile");
+INSERT INTO tuned_item(property, item) VALUES('/etc/profile', 'Profile');
 
 -- collection table
-INSERT INTO collection(name, module, purpose, metrics) VALUES("cpu", "CPU", "STAT", "--interval={interval}; --fields=usr --fields=nice --fields=sys --fields=iowait --fields=irq --fields=soft --fields=steal --fields=guest --threshold=30 --fields=util --fields=cutil");
-INSERT INTO collection(name, module, purpose, metrics) VALUES("storage", "STORAGE", "STAT", "--interval={interval};--device={disk} --fields=rs --fields=ws --fields=rMBs --fields=wMBs --fields=rrqm --fields=wrqm --fields=rareq-sz --fields=wareq-sz --fields=r_await --fields=w_await --fields=util --fields=aqu-sz");
-INSERT INTO collection(name, module, purpose, metrics) VALUES("network", "NET", "STAT", "--interval={interval};--nic={network} --fields=rxkBs --fields=txkBs --fields=rxpcks --fields=txpcks --fields=ifutil");
-INSERT INTO collection(name, module, purpose, metrics) VALUES("network-err", "NET", "ESTAT", "--interval={interval};--nic={network} --fields=errs --fields=util");
-INSERT INTO collection(name, module, purpose, metrics) VALUES("mem.band", "MEM", "BANDWIDTH", "--interval={interval};--fields=Total_Util");
-INSERT INTO collection(name, module, purpose, metrics) VALUES("perf", "PERF", "STAT", "--interval={interval};--fields=IPC --fields=CACHE-MISS-RATIO --fields=MPKI --fields=ITLB-LOAD-MISS-RATIO --fields=DTLB-LOAD-MISS-RATIO --fields=SBPI --fields=SBPC");
-INSERT INTO collection(name, module, purpose, metrics) VALUES("vmstat", "MEM", "VMSTAT", "--interval={interval};--fields=procs.b --fields=memory.swpd --fields=io.bo --fields=system.in --fields=system.cs --fields=util.swap --fields=util.cpu --fields=procs.r");
-INSERT INTO collection(name, module, purpose, metrics) VALUES("sys.task", "SYS", "TASKS", "--interval={interval};--fields=procs --fields=cswchs");
-INSERT INTO collection(name, module, purpose, metrics) VALUES("sys.ldavg", "SYS", "LDAVG", "--interval={interval};--fields=runq-sz --fields=plist-sz --fields=ldavg-1 --fields=ldavg-5");
-INSERT INTO collection(name, module, purpose, metrics) VALUES("file.util", "SYS", "FDUTIL", "--interval={interval};--fields=fd-util");
+INSERT INTO collection(name, module, purpose, metrics) VALUES('cpu', 'CPU', 'STAT', '--interval={interval}; --fields=usr --fields=nice --fields=sys --fields=iowait --fields=irq --fields=soft --fields=steal --fields=guest --threshold=30 --fields=util --fields=cutil');
+INSERT INTO collection(name, module, purpose, metrics) VALUES('storage', 'STORAGE', 'STAT', '--interval={interval};--device={disk} --fields=rs --fields=ws --fields=rMBs --fields=wMBs --fields=rrqm --fields=wrqm --fields=rareq-sz --fields=wareq-sz --fields=r_await --fields=w_await --fields=util --fields=aqu-sz');
+INSERT INTO collection(name, module, purpose, metrics) VALUES('network', 'NET', 'STAT', '--interval={interval};--nic={network} --fields=rxkBs --fields=txkBs --fields=rxpcks --fields=txpcks --fields=ifutil');
+INSERT INTO collection(name, module, purpose, metrics) VALUES('network-err', 'NET', 'ESTAT', '--interval={interval};--nic={network} --fields=errs --fields=util');
+INSERT INTO collection(name, module, purpose, metrics) VALUES('mem.band', 'MEM', 'BANDWIDTH', '--interval={interval};--fields=Total_Util');
+INSERT INTO collection(name, module, purpose, metrics) VALUES('perf', 'PERF', 'STAT', '--interval={interval};--fields=IPC --fields=CACHE-MISS-RATIO --fields=MPKI --fields=ITLB-LOAD-MISS-RATIO --fields=DTLB-LOAD-MISS-RATIO --fields=SBPI --fields=SBPC');
+INSERT INTO collection(name, module, purpose, metrics) VALUES('vmstat', 'MEM', 'VMSTAT', '--interval={interval};--fields=procs.b --fields=memory.swpd --fields=io.bo --fields=system.in --fields=system.cs --fields=util.swap --fields=util.cpu --fields=procs.r');
+INSERT INTO collection(name, module, purpose, metrics) VALUES('sys.task', 'SYS', 'TASKS', '--interval={interval};--fields=procs --fields=cswchs');
+INSERT INTO collection(name, module, purpose, metrics) VALUES('sys.ldavg', 'SYS', 'LDAVG', '--interval={interval};--fields=runq-sz --fields=plist-sz --fields=ldavg-1 --fields=ldavg-5');
+INSERT INTO collection(name, module, purpose, metrics) VALUES('file.util', 'SYS', 'FDUTIL', '--interval={interval};--fields=fd-util');
 
 -- Dynamic_tuned table
-INSERT INTO rule_tuned(name, class, expression, action, opposite_action, monitor, field) VALUES("hpre", "webserver", "object in ('libssl', 'libcrypto')", "openssl_hpre=1", "openssl_hpre=0","PERF.TOP", ";--fields=overhead --fields=object --fields=symbol --addr-merge=0x3f");
+INSERT INTO rule_tuned(name, class, expression, action, opposite_action, monitor, field) VALUES('hpre', 'webserver', 'object in (''libssl'', ''libcrypto'')', 'openssl_hpre=1', 'openssl_hpre=0','PERF.TOP', ';--fields=overhead --fields=object --fields=symbol --addr-merge=0x3f');
 
 -- AI search table
--- INSERT INTO tuned (class, name, type, value, range) VALUES("single_computer_intensive_jobs", "prefetech", "ENUM", "off", "on,off" );
+-- INSERT INTO tuned (class, name, type, value, range) VALUES('single_computer_intensive_jobs', 'prefetech', 'ENUM', 'off', 'on,off' );
 
 -- Schedule table
-INSERT INTO schedule (type, strategy) VALUES("all", "auto");
+INSERT INTO schedule (type, strategy) VALUES('all', 'auto');
-- 
2.33.0

