From 4c3e5be27dd56bb67f7e259f6f24dcb392b3aaa2 Mon Sep 17 00:00:00 2001
From: mengqinggang <mengqinggang@loongson.cn>
Date: Fri, 5 Jul 2024 10:40:33 +0800
Subject: [PATCH 10/15] LoongArch: Add cfi instructions for _dl_tlsdesc_dynamic

In _dl_tlsdesc_dynamic, there are three 'addi.d sp, sp, -size'
instructions to allocate stack size for Float/LSX/LASX registers.
Every 'addi.d sp, sp, -size' needs a cfi_adjust_cfa_offset because
of sp is used to compute CFA. But only one 'addi.d sp, sp, -size'
will be run according to HWCAP value. And all cfi_adjust_cfa_offset
will be executed in stack unwinding, it result in incorrect CFA.

Change _dl_tlsdesc_dynamic to _dl_tlsdesc_dynamic,
_dl_tlsdesc_dynamic_lsx and _dl_tlsdesc_dynamic_lasx.
Conflicting cfi instructions can be distributed to the three functions.
And cfi instructions can correspond to stack down instructions.
---
 sysdeps/loongarch/dl-machine.h         |   7 +
 sysdeps/loongarch/dl-tlsdesc-dynamic.h | 225 ++++++++++++++
 sysdeps/loongarch/dl-tlsdesc.S         | 386 ++-----------------------
 sysdeps/loongarch/dl-tlsdesc.h         |   4 +
 sysdeps/loongarch/tlsdesc.sym          |   9 -
 5 files changed, 258 insertions(+), 373 deletions(-)
 create mode 100644 sysdeps/loongarch/dl-tlsdesc-dynamic.h

diff --git a/sysdeps/loongarch/dl-machine.h b/sysdeps/loongarch/dl-machine.h
index 222d51a8..d934c77f 100644
--- a/sysdeps/loongarch/dl-machine.h
+++ b/sysdeps/loongarch/dl-machine.h
@@ -222,6 +222,13 @@ elf_machine_rela (struct link_map *map, struct r_scope_elem *scope[],
 	      {
 		td->arg = _dl_make_tlsdesc_dynamic (sym_map,
 			      sym->st_value + reloc->r_addend);
+# ifndef __loongarch_soft_float
+		if (RTLD_SUPPORT_LASX)
+		  td->entry = _dl_tlsdesc_dynamic_lasx;
+		else if (RTLD_SUPPORT_LSX)
+		  td->entry = _dl_tlsdesc_dynamic_lsx;
+		else
+# endif
 		td->entry = _dl_tlsdesc_dynamic;
 	      }
 	    else
diff --git a/sysdeps/loongarch/dl-tlsdesc-dynamic.h b/sysdeps/loongarch/dl-tlsdesc-dynamic.h
new file mode 100644
index 00000000..d10f4a88
--- /dev/null
+++ b/sysdeps/loongarch/dl-tlsdesc-dynamic.h
@@ -0,0 +1,225 @@
+/* Thread-local storage handling in the ELF dynamic linker.
+   LoongArch version.
+   Copyright (C) 2024 Free Software Foundation, Inc.
+
+   This file is part of the GNU C Library.
+
+   The GNU C Library is free software; you can redistribute it and/or
+   modify it under the terms of the GNU Lesser General Public
+   License as published by the Free Software Foundation; either
+   version 2.1 of the License, or (at your option) any later version.
+
+   The GNU C Library is distributed in the hope that it will be useful,
+   but WITHOUT ANY WARRANTY; without even the implied warranty of
+   MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the GNU
+   Lesser General Public License for more details.
+
+   You should have received a copy of the GNU Lesser General Public
+   License along with the GNU C Library; if not, see
+   <https://www.gnu.org/licenses/>.  */
+
+#define FRAME_SIZE	  (-((-14 * SZREG) & ALMASK))
+#define FRAME_SIZE_LSX	  (-((-32 * SZVREG) & ALMASK))
+#define FRAME_SIZE_LASX	  (-((-32 * SZXREG) & ALMASK))
+#define FRAME_SIZE_FLOAT  (-((-24 * SZFREG) & ALMASK))
+
+	/* Handler for dynamic TLS symbols.
+	   Prototype:
+	   _dl_tlsdesc_dynamic (tlsdesc *) ;
+
+	   The second word of the descriptor points to a
+	   tlsdesc_dynamic_arg structure.
+
+	   Returns the offset between the thread pointer and the
+	   object referenced by the argument.
+
+	   ptrdiff_t
+	   _dl_tlsdesc_dynamic (struct tlsdesc *tdp)
+	   {
+	     struct tlsdesc_dynamic_arg *td = tdp->arg;
+	     dtv_t *dtv = *(dtv_t **)((char *)__thread_pointer - SIZE_OF_TCB);
+	     if (__glibc_likely (td->gen_count <= dtv[0].counter
+		&& (dtv[td->tlsinfo.ti_module].pointer.val
+		    != TLS_DTV_UNALLOCATED),
+		1))
+	       return dtv[td->tlsinfo.ti_module].pointer.val
+		+ td->tlsinfo.ti_offset
+		- __thread_pointer;
+
+	     return ___tls_get_addr (&td->tlsinfo) - __thread_pointer;
+	   }  */
+	.hidden _dl_tlsdesc_dynamic
+	.global	_dl_tlsdesc_dynamic
+	.type	_dl_tlsdesc_dynamic,%function
+	cfi_startproc
+	.align 2
+_dl_tlsdesc_dynamic:
+	/* Save just enough registers to support fast path, if we fall
+	   into slow path we will save additional registers.  */
+	ADDI	sp, sp, -32
+	cfi_adjust_cfa_offset (32)
+	REG_S	t0, sp, 0
+	REG_S	t1, sp, 8
+	REG_S	t2, sp, 16
+	cfi_rel_offset (12, 0)
+	cfi_rel_offset (13, 8)
+	cfi_rel_offset (14, 16)
+
+/* Runtime Storage Layout of Thread-Local Storage
+   TP point to the start of TLS block.
+
+				      dtv
+Low address	TCB ----------------> dtv0(counter)
+	 TP -->	static_block0  <----- dtv1
+		static_block1  <----- dtv2
+		static_block2  <----- dtv3
+		dynamic_block0 <----- dtv4
+Hign address	dynamic_block1 <----- dtv5  */
+
+	REG_L	t0, tp, -SIZE_OF_TCB	  /* t0 = dtv */
+	REG_L	a0, a0, TLSDESC_ARG	  /* a0(td) = tdp->arg */
+	REG_L	t1, a0, TLSDESC_GEN_COUNT /* t1 = td->gen_count */
+	REG_L	t2, t0, DTV_COUNTER	  /* t2 = dtv[0].counter */
+	/* If dtv[0].counter < td->gen_count, goto slow path.  */
+	bltu	t2, t1, .Lslow
+
+	REG_L	t1, a0, TLSDESC_MODID /* t1 = td->tlsinfo.ti_module */
+	/* t1 = t1 * sizeof(dtv_t) = t1 * (2 * sizeof(void*)) */
+	slli.d	t1, t1, 4
+	add.d	t1, t1, t0  /* t1 = dtv[td->tlsinfo.ti_module] */
+	REG_L	t1, t1, 0   /* t1 = dtv[td->tlsinfo.ti_module].pointer.val */
+	li.d	t2, TLS_DTV_UNALLOCATED
+	/* If dtv[td->tlsinfo.ti_module].pointer.val is TLS_DTV_UNALLOCATED,
+	   goto slow path.  */
+	beq	t1, t2, .Lslow
+
+	cfi_remember_state
+	REG_L	t2, a0, TLSDESC_MODOFF	/* t2 = td->tlsinfo.ti_offset */
+	/* dtv[td->tlsinfo.ti_module].pointer.val + td->tlsinfo.ti_offset */
+	add.d	a0, t1, t2
+.Lret:
+	sub.d	a0, a0, tp
+	REG_L	t0, sp, 0
+	REG_L	t1, sp, 8
+	REG_L	t2, sp, 16
+	ADDI	sp, sp, 32
+	cfi_adjust_cfa_offset (-32)
+	RET
+
+.Lslow:
+	/* This is the slow path.  We need to call __tls_get_addr() which
+	   means we need to save and restore all the register that the
+	   callee will trash.  */
+
+	/* Save the remaining registers that we must treat as caller save.  */
+	cfi_restore_state
+	ADDI	sp, sp, -FRAME_SIZE
+	cfi_adjust_cfa_offset (FRAME_SIZE)
+	REG_S	ra, sp, 0 * SZREG
+	REG_S	a1, sp, 1 * SZREG
+	REG_S	a2, sp, 2 * SZREG
+	REG_S	a3, sp, 3 * SZREG
+	REG_S	a4, sp, 4 * SZREG
+	REG_S	a5, sp, 5 * SZREG
+	REG_S	a6, sp, 6 * SZREG
+	REG_S	a7, sp, 7 * SZREG
+	REG_S	t3, sp, 8 * SZREG
+	REG_S	t4, sp, 9 * SZREG
+	REG_S	t5, sp, 10 * SZREG
+	REG_S	t6, sp, 11 * SZREG
+	REG_S	t7, sp, 12 * SZREG
+	REG_S	t8, sp, 13 * SZREG
+	cfi_rel_offset (1, 0 * SZREG)
+	cfi_rel_offset (5, 1 * SZREG)
+	cfi_rel_offset (6, 2 * SZREG)
+	cfi_rel_offset (7, 3 * SZREG)
+	cfi_rel_offset (8, 4 * SZREG)
+	cfi_rel_offset (9, 5 * SZREG)
+	cfi_rel_offset (10, 6 * SZREG)
+	cfi_rel_offset (11, 7 * SZREG)
+	cfi_rel_offset (15, 8 * SZREG)
+	cfi_rel_offset (16, 9 * SZREG)
+	cfi_rel_offset (17, 10 * SZREG)
+	cfi_rel_offset (18, 11 * SZREG)
+	cfi_rel_offset (19, 12 * SZREG)
+	cfi_rel_offset (20, 13 * SZREG)
+
+#ifndef __loongarch_soft_float
+
+	/* Save fcsr0 register.
+	   Only one physical fcsr0 register, fcsr1-fcsr3 are aliases
+	   of some fields in fcsr0.  */
+	movfcsr2gr  t0, fcsr0
+	st.w	t0, sp, FRAME_SIZE + 24 /* Use the spare slot above t2.  */
+
+#ifdef USE_LASX
+  #define V_REG_S xvst
+  #define V_REG_L xvld
+  #define V_SPACE FRAME_SIZE_LASX
+  #define V_REG(n) $xr##n
+  #define V_REGS 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,  \
+		 17,18,19,20,21,22,23,24,25,26,27,28,29,30,31
+  #define V_REGSZ SZXREG
+#elif defined USE_LSX
+  #define V_REG_S vst
+  #define V_REG_L vld
+  #define V_SPACE FRAME_SIZE_LSX
+  #define V_REG(n) $vr##n
+  #define V_REGS 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,  \
+		 17,18,19,20,21,22,23,24,25,26,27,28,29,30,31
+  #define V_REGSZ SZVREG
+#else
+  #define V_REG_S fst.d
+  #define V_REG_L fld.d
+  #define V_SPACE FRAME_SIZE_FLOAT
+  #define V_REG(n) $f##n
+  #define V_REGS 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23
+  #define V_REGSZ SZFREG
+#endif
+
+	ADDI	sp, sp, -V_SPACE
+	cfi_adjust_cfa_offset (V_SPACE)
+	.irp	i,V_REGS
+        V_REG_S	V_REG(\i), sp, \i * V_REGSZ
+	.endr
+
+#endif /* #ifndef __loongarch_soft_float */
+
+	bl	HIDDEN_JUMPTARGET(__tls_get_addr)
+	ADDI	a0, a0, -TLS_DTV_OFFSET
+
+#ifndef __loongarch_soft_float
+
+	.irp	i,V_REGS
+	V_REG_L	V_REG(\i), sp, \i * V_REGSZ
+	.endr
+	ADDI	sp, sp, V_SPACE
+	cfi_adjust_cfa_offset (-V_SPACE)
+
+	/* Restore fcsr0 register.  */
+	ld.w	t0, sp, FRAME_SIZE + 24
+	movgr2fcsr  fcsr0, t0
+
+#endif /* #ifndef __loongarch_soft_float */
+
+	REG_L	ra, sp, 0 * SZREG
+	REG_L	a1, sp, 1 * SZREG
+	REG_L	a2, sp, 2 * SZREG
+	REG_L	a3, sp, 3 * SZREG
+	REG_L	a4, sp, 4 * SZREG
+	REG_L	a5, sp, 5 * SZREG
+	REG_L	a6, sp, 6 * SZREG
+	REG_L	a7, sp, 7 * SZREG
+	REG_L	t3, sp, 8 * SZREG
+	REG_L	t4, sp, 9 * SZREG
+	REG_L	t5, sp, 10 * SZREG
+	REG_L	t6, sp, 11 * SZREG
+	REG_L	t7, sp, 12 * SZREG
+	REG_L	t8, sp, 13 * SZREG
+	ADDI	sp, sp, FRAME_SIZE
+	cfi_adjust_cfa_offset (-FRAME_SIZE)
+
+	b	.Lret
+	cfi_endproc
+	.size	_dl_tlsdesc_dynamic, .-_dl_tlsdesc_dynamic
+	.hidden HIDDEN_JUMPTARGET(__tls_get_addr)
diff --git a/sysdeps/loongarch/dl-tlsdesc.S b/sysdeps/loongarch/dl-tlsdesc.S
index a6627cc7..b6cfd612 100644
--- a/sysdeps/loongarch/dl-tlsdesc.S
+++ b/sysdeps/loongarch/dl-tlsdesc.S
@@ -59,376 +59,34 @@ _dl_tlsdesc_undefweak:
 	cfi_endproc
 	.size	_dl_tlsdesc_undefweak, .-_dl_tlsdesc_undefweak
 
-
 #ifdef SHARED
 
-#define FRAME_SIZE	  (-((-14 * SZREG) & ALMASK))
-#define FRAME_SIZE_LSX	  (-((-32 * SZVREG) & ALMASK))
-#define FRAME_SIZE_LASX	  (-((-32 * SZXREG) & ALMASK))
-#define FRAME_SIZE_FLOAT  (-((-24 * SZFREG) & ALMASK))
-
-	/* Handler for dynamic TLS symbols.
-	   Prototype:
-	   _dl_tlsdesc_dynamic (tlsdesc *) ;
-
-	   The second word of the descriptor points to a
-	   tlsdesc_dynamic_arg structure.
-
-	   Returns the offset between the thread pointer and the
-	   object referenced by the argument.
-
-	   ptrdiff_t
-	   _dl_tlsdesc_dynamic (struct tlsdesc *tdp)
-	   {
-	     struct tlsdesc_dynamic_arg *td = tdp->arg;
-	     dtv_t *dtv = *(dtv_t **)((char *)__thread_pointer - SIZE_OF_TCB);
-	     if (__glibc_likely (td->gen_count <= dtv[0].counter
-		&& (dtv[td->tlsinfo.ti_module].pointer.val
-		    != TLS_DTV_UNALLOCATED),
-		1))
-	       return dtv[td->tlsinfo.ti_module].pointer.val
-		+ td->tlsinfo.ti_offset
-		- __thread_pointer;
-
-	     return ___tls_get_addr (&td->tlsinfo) - __thread_pointer;
-	   }  */
-	.hidden _dl_tlsdesc_dynamic
-	.global	_dl_tlsdesc_dynamic
-	.type	_dl_tlsdesc_dynamic,%function
-	cfi_startproc
-	.align 2
-_dl_tlsdesc_dynamic:
-	/* Save just enough registers to support fast path, if we fall
-	   into slow path we will save additional registers.  */
-	ADDI	sp, sp, -32
-	REG_S	t0, sp, 0
-	REG_S	t1, sp, 8
-	REG_S	t2, sp, 16
-
-/* Runtime Storage Layout of Thread-Local Storage
-   TP point to the start of TLS block.
-
-				      dtv
-Low address	TCB ----------------> dtv0(counter)
-	 TP -->	static_block0  <----- dtv1
-		static_block1  <----- dtv2
-		static_block2  <----- dtv3
-		dynamic_block0 <----- dtv4
-Hign address	dynamic_block1 <----- dtv5  */
-
-	REG_L	t0, tp, -SIZE_OF_TCB	  /* t0 = dtv */
-	REG_L	a0, a0, TLSDESC_ARG	  /* a0(td) = tdp->arg */
-	REG_L	t1, a0, TLSDESC_GEN_COUNT /* t1 = td->gen_count */
-	REG_L	t2, t0, DTV_COUNTER	  /* t2 = dtv[0].counter */
-	/* If dtv[0].counter < td->gen_count, goto slow path.  */
-	bltu	t2, t1, .Lslow
-
-	REG_L	t1, a0, TLSDESC_MODID /* t1 = td->tlsinfo.ti_module */
-	/* t1 = t1 * sizeof(dtv_t) = t1 * (2 * sizeof(void*)) */
-	slli.d	t1, t1, 4
-	add.d	t1, t1, t0  /* t1 = dtv[td->tlsinfo.ti_module] */
-	REG_L	t1, t1, 0   /* t1 = dtv[td->tlsinfo.ti_module].pointer.val */
-	li.d	t2, TLS_DTV_UNALLOCATED
-	/* If dtv[td->tlsinfo.ti_module].pointer.val is TLS_DTV_UNALLOCATED,
-	   goto slow path.  */
-	beq	t1, t2, .Lslow
-
-	REG_L	t2, a0, TLSDESC_MODOFF	/* t2 = td->tlsinfo.ti_offset */
-	/* dtv[td->tlsinfo.ti_module].pointer.val + td->tlsinfo.ti_offset */
-	add.d	a0, t1, t2
-.Lret:
-	sub.d	a0, a0, tp
-	REG_L	t0, sp, 0
-	REG_L	t1, sp, 8
-	REG_L	t2, sp, 16
-	ADDI	sp, sp, 32
-	RET
-
-.Lslow:
-	/* This is the slow path. We need to call __tls_get_addr() which
-	   means we need to save and restore all the register that the
-	   callee will trash.  */
-
-	/* Save the remaining registers that we must treat as caller save.  */
-	ADDI	sp, sp, -FRAME_SIZE
-	REG_S	ra, sp, 0 * SZREG
-	REG_S	a1, sp, 1 * SZREG
-	REG_S	a2, sp, 2 * SZREG
-	REG_S	a3, sp, 3 * SZREG
-	REG_S	a4, sp, 4 * SZREG
-	REG_S	a5, sp, 5 * SZREG
-	REG_S	a6, sp, 6 * SZREG
-	REG_S	a7, sp, 7 * SZREG
-	REG_S	t3, sp, 8 * SZREG
-	REG_S	t4, sp, 9 * SZREG
-	REG_S	t5, sp, 10 * SZREG
-	REG_S	t6, sp, 11 * SZREG
-	REG_S	t7, sp, 12 * SZREG
-	REG_S	t8, sp, 13 * SZREG
-
 #ifndef __loongarch_soft_float
 
-	/* Save fcsr0 register.
-	   Only one physical fcsr0 register, fcsr1-fcsr3 are aliases
-	   of some fields in fcsr0.  */
-	movfcsr2gr  t0, fcsr0
-	st.w	t0, sp, FRAME_SIZE + 24 /* Use the spare slot above t2 */
-
-	/* Whether support LASX.  */
-	la.global   t0, _rtld_global_ro
-	REG_L	t0, t0, GLRO_DL_HWCAP_OFFSET
-	andi	t1, t0, HWCAP_LOONGARCH_LASX
-	beqz	t1, .Llsx
-
-	/* Save 256-bit vector registers.
-	   FIXME: Without vector ABI, save all vector registers.  */
-	ADDI	sp, sp, -FRAME_SIZE_LASX
-	xvst	xr0, sp, 0*SZXREG
-	xvst	xr1, sp, 1*SZXREG
-	xvst	xr2, sp, 2*SZXREG
-	xvst	xr3, sp, 3*SZXREG
-	xvst	xr4, sp, 4*SZXREG
-	xvst	xr5, sp, 5*SZXREG
-	xvst	xr6, sp, 6*SZXREG
-	xvst	xr7, sp, 7*SZXREG
-	xvst	xr8, sp, 8*SZXREG
-	xvst	xr9, sp, 9*SZXREG
-	xvst	xr10, sp, 10*SZXREG
-	xvst	xr11, sp, 11*SZXREG
-	xvst	xr12, sp, 12*SZXREG
-	xvst	xr13, sp, 13*SZXREG
-	xvst	xr14, sp, 14*SZXREG
-	xvst	xr15, sp, 15*SZXREG
-	xvst	xr16, sp, 16*SZXREG
-	xvst	xr17, sp, 17*SZXREG
-	xvst	xr18, sp, 18*SZXREG
-	xvst	xr19, sp, 19*SZXREG
-	xvst	xr20, sp, 20*SZXREG
-	xvst	xr21, sp, 21*SZXREG
-	xvst	xr22, sp, 22*SZXREG
-	xvst	xr23, sp, 23*SZXREG
-	xvst	xr24, sp, 24*SZXREG
-	xvst	xr25, sp, 25*SZXREG
-	xvst	xr26, sp, 26*SZXREG
-	xvst	xr27, sp, 27*SZXREG
-	xvst	xr28, sp, 28*SZXREG
-	xvst	xr29, sp, 29*SZXREG
-	xvst	xr30, sp, 30*SZXREG
-	xvst	xr31, sp, 31*SZXREG
-	b	    .Ltga
-
-.Llsx:
-	/* Whether support LSX.  */
-	andi	t1, t0, HWCAP_LOONGARCH_LSX
-	beqz	t1, .Lfloat
-
-	/* Save 128-bit vector registers.  */
-	ADDI	sp, sp, -FRAME_SIZE_LSX
-	vst	vr0, sp, 0*SZVREG
-	vst	vr1, sp, 1*SZVREG
-	vst	vr2, sp, 2*SZVREG
-	vst	vr3, sp, 3*SZVREG
-	vst	vr4, sp, 4*SZVREG
-	vst	vr5, sp, 5*SZVREG
-	vst	vr6, sp, 6*SZVREG
-	vst	vr7, sp, 7*SZVREG
-	vst	vr8, sp, 8*SZVREG
-	vst	vr9, sp, 9*SZVREG
-	vst	vr10, sp, 10*SZVREG
-	vst	vr11, sp, 11*SZVREG
-	vst	vr12, sp, 12*SZVREG
-	vst	vr13, sp, 13*SZVREG
-	vst	vr14, sp, 14*SZVREG
-	vst	vr15, sp, 15*SZVREG
-	vst	vr16, sp, 16*SZVREG
-	vst	vr17, sp, 17*SZVREG
-	vst	vr18, sp, 18*SZVREG
-	vst	vr19, sp, 19*SZVREG
-	vst	vr20, sp, 20*SZVREG
-	vst	vr21, sp, 21*SZVREG
-	vst	vr22, sp, 22*SZVREG
-	vst	vr23, sp, 23*SZVREG
-	vst	vr24, sp, 24*SZVREG
-	vst	vr25, sp, 25*SZVREG
-	vst	vr26, sp, 26*SZVREG
-	vst	vr27, sp, 27*SZVREG
-	vst	vr28, sp, 28*SZVREG
-	vst	vr29, sp, 29*SZVREG
-	vst	vr30, sp, 30*SZVREG
-	vst	vr31, sp, 31*SZVREG
-	b	    .Ltga
-
-.Lfloat:
-	/* Save float registers.  */
-	ADDI	sp, sp, -FRAME_SIZE_FLOAT
-	FREG_S	fa0, sp, 0*SZFREG
-	FREG_S	fa1, sp, 1*SZFREG
-	FREG_S	fa2, sp, 2*SZFREG
-	FREG_S	fa3, sp, 3*SZFREG
-	FREG_S	fa4, sp, 4*SZFREG
-	FREG_S	fa5, sp, 5*SZFREG
-	FREG_S	fa6, sp, 6*SZFREG
-	FREG_S	fa7, sp, 7*SZFREG
-	FREG_S	ft0, sp, 8*SZFREG
-	FREG_S	ft1, sp, 9*SZFREG
-	FREG_S	ft2, sp, 10*SZFREG
-	FREG_S	ft3, sp, 11*SZFREG
-	FREG_S	ft4, sp, 12*SZFREG
-	FREG_S	ft5, sp, 13*SZFREG
-	FREG_S	ft6, sp, 14*SZFREG
-	FREG_S	ft7, sp, 15*SZFREG
-	FREG_S	ft8, sp, 16*SZFREG
-	FREG_S	ft9, sp, 17*SZFREG
-	FREG_S	ft10, sp, 18*SZFREG
-	FREG_S	ft11, sp, 19*SZFREG
-	FREG_S	ft12, sp, 20*SZFREG
-	FREG_S	ft13, sp, 21*SZFREG
-	FREG_S	ft14, sp, 22*SZFREG
-	FREG_S	ft15, sp, 23*SZFREG
-
-#endif /* #ifndef __loongarch_soft_float */
-
-.Ltga:
-	bl	HIDDEN_JUMPTARGET(__tls_get_addr)
-	ADDI	a0, a0, -TLS_DTV_OFFSET
-
-#ifndef __loongarch_soft_float
-
-	la.global   t0, _rtld_global_ro
-	REG_L	t0, t0, GLRO_DL_HWCAP_OFFSET
-	andi	t1, t0, HWCAP_LOONGARCH_LASX
-	beqz	t1, .Llsx1
-
-	/* Restore 256-bit vector registers.  */
-	xvld	xr0, sp, 0*SZXREG
-	xvld	xr1, sp, 1*SZXREG
-	xvld	xr2, sp, 2*SZXREG
-	xvld	xr3, sp, 3*SZXREG
-	xvld	xr4, sp, 4*SZXREG
-	xvld	xr5, sp, 5*SZXREG
-	xvld	xr6, sp, 6*SZXREG
-	xvld	xr7, sp, 7*SZXREG
-	xvld	xr8, sp, 8*SZXREG
-	xvld	xr9, sp, 9*SZXREG
-	xvld	xr10, sp, 10*SZXREG
-	xvld	xr11, sp, 11*SZXREG
-	xvld	xr12, sp, 12*SZXREG
-	xvld	xr13, sp, 13*SZXREG
-	xvld	xr14, sp, 14*SZXREG
-	xvld	xr15, sp, 15*SZXREG
-	xvld	xr16, sp, 16*SZXREG
-	xvld	xr17, sp, 17*SZXREG
-	xvld	xr18, sp, 18*SZXREG
-	xvld	xr19, sp, 19*SZXREG
-	xvld	xr20, sp, 20*SZXREG
-	xvld	xr21, sp, 21*SZXREG
-	xvld	xr22, sp, 22*SZXREG
-	xvld	xr23, sp, 23*SZXREG
-	xvld	xr24, sp, 24*SZXREG
-	xvld	xr25, sp, 25*SZXREG
-	xvld	xr26, sp, 26*SZXREG
-	xvld	xr27, sp, 27*SZXREG
-	xvld	xr28, sp, 28*SZXREG
-	xvld	xr29, sp, 29*SZXREG
-	xvld	xr30, sp, 30*SZXREG
-	xvld	xr31, sp, 31*SZXREG
-	ADDI	sp, sp, FRAME_SIZE_LASX
-	b .Lfcsr
-
-.Llsx1:
-	andi	t1, t0, HWCAP_LOONGARCH_LSX
-	beqz	t1, .Lfloat1
-
-	/* Restore 128-bit vector registers.  */
-	vld	vr0, sp, 0*SZVREG
-	vld	vr1, sp, 1*SZVREG
-	vld	vr2, sp, 2*SZVREG
-	vld	vr3, sp, 3*SZVREG
-	vld	vr4, sp, 4*SZVREG
-	vld	vr5, sp, 5*SZVREG
-	vld	vr6, sp, 6*SZVREG
-	vld	vr7, sp, 7*SZVREG
-	vld	vr8, sp, 8*SZVREG
-	vld	vr9, sp, 9*SZVREG
-	vld	vr10, sp, 10*SZVREG
-	vld	vr11, sp, 11*SZVREG
-	vld	vr12, sp, 12*SZVREG
-	vld	vr13, sp, 13*SZVREG
-	vld	vr14, sp, 14*SZVREG
-	vld	vr15, sp, 15*SZVREG
-	vld	vr16, sp, 16*SZVREG
-	vld	vr17, sp, 17*SZVREG
-	vld	vr18, sp, 18*SZVREG
-	vld	vr19, sp, 19*SZVREG
-	vld	vr20, sp, 20*SZVREG
-	vld	vr21, sp, 21*SZVREG
-	vld	vr22, sp, 22*SZVREG
-	vld	vr23, sp, 23*SZVREG
-	vld	vr24, sp, 24*SZVREG
-	vld	vr25, sp, 25*SZVREG
-	vld	vr26, sp, 26*SZVREG
-	vld	vr27, sp, 27*SZVREG
-	vld	vr28, sp, 28*SZVREG
-	vld	vr29, sp, 29*SZVREG
-	vld	vr30, sp, 30*SZVREG
-	vld	vr31, sp, 31*SZVREG
-	ADDI	sp, sp, FRAME_SIZE_LSX
-	b	    .Lfcsr
-
-.Lfloat1:
-	/* Restore float registers.  */
-	FREG_L	fa0, sp, 0*SZFREG
-	FREG_L	fa1, sp, 1*SZFREG
-	FREG_L	fa2, sp, 2*SZFREG
-	FREG_L	fa3, sp, 3*SZFREG
-	FREG_L	fa4, sp, 4*SZFREG
-	FREG_L	fa5, sp, 5*SZFREG
-	FREG_L	fa6, sp, 6*SZFREG
-	FREG_L	fa7, sp, 7*SZFREG
-	FREG_L	ft0, sp, 8*SZFREG
-	FREG_L	ft1, sp, 9*SZFREG
-	FREG_L	ft2, sp, 10*SZFREG
-	FREG_L	ft3, sp, 11*SZFREG
-	FREG_L	ft4, sp, 12*SZFREG
-	FREG_L	ft5, sp, 13*SZFREG
-	FREG_L	ft6, sp, 14*SZFREG
-	FREG_L	ft7, sp, 15*SZFREG
-	FREG_L	ft8, sp, 16*SZFREG
-	FREG_L	ft9, sp, 17*SZFREG
-	FREG_L	ft10, sp, 18*SZFREG
-	FREG_L	ft11, sp, 19*SZFREG
-	FREG_L	ft12, sp, 20*SZFREG
-	FREG_L	ft13, sp, 21*SZFREG
-	FREG_L	ft14, sp, 22*SZFREG
-	FREG_L	ft15, sp, 23*SZFREG
-	ADDI	sp, sp, FRAME_SIZE_FLOAT
-
-.Lfcsr:
-	/* Restore fcsr0 register.  */
-	ld.w	t0, sp, FRAME_SIZE + 24
-	movgr2fcsr  fcsr0, t0
+#define USE_LASX
+#define _dl_tlsdesc_dynamic _dl_tlsdesc_dynamic_lasx
+#define Lret Lret_lasx
+#define Lslow Lslow_lasx
+#include "dl-tlsdesc-dynamic.h"
+#undef FRAME_SIZE
+#undef USE_LASX
+#undef _dl_tlsdesc_dynamic
+#undef Lret
+#undef Lslow
+
+#define USE_LSX
+#define _dl_tlsdesc_dynamic _dl_tlsdesc_dynamic_lsx
+#define Lret Lret_lsx
+#define Lslow Lslow_lsx
+#include "dl-tlsdesc-dynamic.h"
+#undef FRAME_SIZE
+#undef USE_LSX
+#undef _dl_tlsdesc_dynamic
+#undef Lret
+#undef Lslow
 
 #endif /* #ifndef __loongarch_soft_float */
 
-	REG_L	ra, sp, 0 * SZREG
-	REG_L	a1, sp, 1 * SZREG
-	REG_L	a2, sp, 2 * SZREG
-	REG_L	a3, sp, 3 * SZREG
-	REG_L	a4, sp, 4 * SZREG
-	REG_L	a5, sp, 5 * SZREG
-	REG_L	a6, sp, 6 * SZREG
-	REG_L	a7, sp, 7 * SZREG
-	REG_L	t3, sp, 8 * SZREG
-	REG_L	t4, sp, 9 * SZREG
-	REG_L	t5, sp, 10 * SZREG
-	REG_L	t6, sp, 11 * SZREG
-	REG_L	t7, sp, 12 * SZREG
-	REG_L	t8, sp, 13 * SZREG
-	ADDI	sp, sp, FRAME_SIZE
-
-	b	.Lret
-	cfi_endproc
-	.size	_dl_tlsdesc_dynamic, .-_dl_tlsdesc_dynamic
-	.hidden HIDDEN_JUMPTARGET(__tls_get_addr)
+#include "dl-tlsdesc-dynamic.h"
 
 #endif /* #ifdef SHARED */
diff --git a/sysdeps/loongarch/dl-tlsdesc.h b/sysdeps/loongarch/dl-tlsdesc.h
index ff8c69cb..45c43a5b 100644
--- a/sysdeps/loongarch/dl-tlsdesc.h
+++ b/sysdeps/loongarch/dl-tlsdesc.h
@@ -43,6 +43,10 @@ extern ptrdiff_t attribute_hidden _dl_tlsdesc_undefweak (struct tlsdesc *);
 
 #ifdef SHARED
 extern void *_dl_make_tlsdesc_dynamic (struct link_map *, size_t);
+#ifndef __loongarch_soft_float
+extern ptrdiff_t attribute_hidden _dl_tlsdesc_dynamic_lasx (struct tlsdesc *);
+extern ptrdiff_t attribute_hidden _dl_tlsdesc_dynamic_lsx (struct tlsdesc *);
+#endif
 extern ptrdiff_t attribute_hidden _dl_tlsdesc_dynamic (struct tlsdesc *);
 #endif
 
diff --git a/sysdeps/loongarch/tlsdesc.sym b/sysdeps/loongarch/tlsdesc.sym
index 213d0b30..9f80fcec 100644
--- a/sysdeps/loongarch/tlsdesc.sym
+++ b/sysdeps/loongarch/tlsdesc.sym
@@ -4,12 +4,6 @@
 #include <link.h>
 #include <dl-tlsdesc.h>
 
-#define SHARED 1
-
-#include <ldsodefs.h>
-
-#define GLRO_offsetof(name) offsetof (struct rtld_global_ro, _##name)
-
 --
 
 -- Abuse tls.h macros to derive offsets relative to the thread register.
@@ -23,6 +17,3 @@ DTV_COUNTER		offsetof(dtv_t, counter)
 TLS_DTV_UNALLOCATED	TLS_DTV_UNALLOCATED
 TLS_DTV_OFFSET		TLS_DTV_OFFSET
 SIZE_OF_TCB		sizeof(tcbhead_t)
-GLRO_DL_HWCAP_OFFSET    GLRO_offsetof (dl_hwcap)
-HWCAP_LOONGARCH_LSX	HWCAP_LOONGARCH_LSX
-HWCAP_LOONGARCH_LASX	HWCAP_LOONGARCH_LASX
-- 
2.43.0

