From 369df8e3006000a4acacc674f5882d8729781811 Mon Sep 17 00:00:00 2001
From: Michael Chang <mchang@suse.com>
Date: Sun, 10 Jul 2016 23:46:31 +0800
Subject: [PATCH 7/8] efinet: Setting network from UEFI device path

The PXE Base Code protocol used to obtain cached PXE DHCPACK packet is no
longer provided for HTTP Boot. Instead, we have to get the HTTP boot
information from the device path nodes defined in following UEFI Specification
sections.

 9.3.5.12 IPv4 Device Path
 9.3.5.13 IPv6 Device Path
 9.3.5.23 Uniform Resource Identifiers (URI) Device Path

This patch basically does:

include/grub/efi/api.h:
Add new structure of Uniform Resource Identifiers (URI) Device Path

grub-core/net/drivers/efi/efinet.c:
Check if PXE Base Code is available, if not it will try to obtain the netboot
information from the device path where the image booted from. The DHCPACK
packet is recoverd from the information in device patch and feed into the same
DHCP packet processing functions to ensure the network interface is setting up
the same way it used to be.

Signed-off-by: Michael Chang <mchang@suse.com>
Signed-off-by: Ken Lin <ken.lin@hpe.com>
---
 grub-core/net/drivers/efi/efinet.c | 268 +++++++++++++++++++++++++++++++++++--
 include/grub/efi/api.h             |  11 ++
 2 files changed, 270 insertions(+), 9 deletions(-)

--- a/grub-core/net/drivers/efi/efinet.c
+++ b/grub-core/net/drivers/efi/efinet.c
@@ -23,6 +23,7 @@
 #include <grub/efi/api.h>
 #include <grub/efi/efi.h>
 #include <grub/i18n.h>
+#include <grub/net/netbuff.h>
 
 GRUB_MOD_LICENSE ("GPLv3+");
 
@@ -341,6 +342,221 @@
   grub_free (handles);
 }
 
+static struct grub_net_buff *
+grub_efinet_create_dhcp_ack_from_device_path (grub_efi_device_path_t *dp, int *use_ipv6)
+{
+  grub_efi_uint16_t uri_len;
+  grub_efi_device_path_t *ldp, *ddp;
+  grub_efi_uri_device_path_t *uri_dp;
+  struct grub_net_buff *nb;
+  grub_err_t err;
+
+  ddp = grub_efi_duplicate_device_path (dp);
+  ldp = grub_efi_find_last_device_path (ddp);
+
+  if (GRUB_EFI_DEVICE_PATH_TYPE (ldp) != GRUB_EFI_MESSAGING_DEVICE_PATH_TYPE
+      || GRUB_EFI_DEVICE_PATH_SUBTYPE (ldp) != GRUB_EFI_URI_DEVICE_PATH_SUBTYPE)
+    {
+      grub_free (ddp);
+      return NULL;
+    }
+
+  uri_len = GRUB_EFI_DEVICE_PATH_LENGTH (ldp) > 4 ? GRUB_EFI_DEVICE_PATH_LENGTH (ldp) - 4  : 0;
+
+  if (!uri_len)
+    {
+      grub_free (ddp);
+      return NULL;
+    }
+
+  uri_dp = (grub_efi_uri_device_path_t *) ldp;
+
+  ldp->type = GRUB_EFI_END_DEVICE_PATH_TYPE;
+  ldp->subtype = GRUB_EFI_END_ENTIRE_DEVICE_PATH_SUBTYPE;
+  ldp->length = sizeof (*ldp);
+
+  ldp = grub_efi_find_last_device_path (ddp);
+
+  if (GRUB_EFI_DEVICE_PATH_TYPE (ldp) != GRUB_EFI_MESSAGING_DEVICE_PATH_TYPE
+      || (GRUB_EFI_DEVICE_PATH_SUBTYPE (ldp) != GRUB_EFI_IPV4_DEVICE_PATH_SUBTYPE
+          && GRUB_EFI_DEVICE_PATH_SUBTYPE (ldp) != GRUB_EFI_IPV6_DEVICE_PATH_SUBTYPE))
+    {
+      grub_free (ddp);
+      return NULL;
+    }
+
+  nb = grub_netbuff_alloc (512);
+  if (!nb)
+    return NULL;
+
+  if (GRUB_EFI_DEVICE_PATH_SUBTYPE (ldp) == GRUB_EFI_IPV4_DEVICE_PATH_SUBTYPE)
+    {
+      grub_efi_ipv4_device_path_t *ipv4 = (grub_efi_ipv4_device_path_t *) ldp;
+      struct grub_net_bootp_packet *bp;
+      grub_uint8_t *ptr;
+
+      bp = (struct grub_net_bootp_packet *) nb->tail;
+      err = grub_netbuff_put (nb, sizeof (*bp) + 4);
+      if (err)
+	{
+	  grub_free (ddp);
+	  grub_netbuff_free (nb);
+	  return NULL;
+	}
+
+      if (sizeof(bp->boot_file) < uri_len)
+	{
+	  grub_free (ddp);
+	  grub_netbuff_free (nb);
+	  return NULL;
+	}
+      grub_memcpy (bp->boot_file, uri_dp->uri, uri_len);
+      grub_memcpy (&bp->your_ip, ipv4->local_ip_address, sizeof (bp->your_ip));
+      grub_memcpy (&bp->server_ip, ipv4->remote_ip_address, sizeof (bp->server_ip));
+
+      bp->vendor[0] = GRUB_NET_BOOTP_RFC1048_MAGIC_0;
+      bp->vendor[1] = GRUB_NET_BOOTP_RFC1048_MAGIC_1;
+      bp->vendor[2] = GRUB_NET_BOOTP_RFC1048_MAGIC_2;
+      bp->vendor[3] = GRUB_NET_BOOTP_RFC1048_MAGIC_3;
+
+      ptr = nb->tail;
+      err = grub_netbuff_put (nb, sizeof (ipv4->subnet_mask) + 2);
+      if (err)
+	{
+	  grub_free (ddp);
+	  grub_netbuff_free (nb);
+	  return NULL;
+	}
+      *ptr++ = GRUB_NET_BOOTP_NETMASK;
+      *ptr++ = sizeof (ipv4->subnet_mask);
+      grub_memcpy (ptr, ipv4->subnet_mask, sizeof (ipv4->subnet_mask));
+
+      ptr = nb->tail;
+      err = grub_netbuff_put (nb, sizeof (ipv4->gateway_ip_address) + 2);
+      if (err)
+	{
+	  grub_free (ddp);
+	  grub_netbuff_free (nb);
+	  return NULL;
+	}
+      *ptr++ = GRUB_NET_BOOTP_ROUTER;
+      *ptr++ = sizeof (ipv4->gateway_ip_address);
+      grub_memcpy (ptr, ipv4->gateway_ip_address, sizeof (ipv4->gateway_ip_address));
+
+      ptr = nb->tail;
+      err = grub_netbuff_put (nb, sizeof ("HTTPClient") + 1);
+      if (err)
+	{
+	  grub_free (ddp);
+	  grub_netbuff_free (nb);
+	  return NULL;
+	}
+      *ptr++ = GRUB_NET_BOOTP_VENDOR_CLASS_IDENTIFIER;
+      *ptr++ = sizeof ("HTTPClient") - 1;
+      grub_memcpy (ptr, "HTTPClient", sizeof ("HTTPClient") - 1);
+
+      ptr = nb->tail;
+      err = grub_netbuff_put (nb, 1);
+      if (err)
+	{
+	  grub_free (ddp);
+	  grub_netbuff_free (nb);
+	  return NULL;
+	}
+      *ptr = GRUB_NET_BOOTP_END;
+      *use_ipv6 = 0;
+
+      ldp->type = GRUB_EFI_END_DEVICE_PATH_TYPE;
+      ldp->subtype = GRUB_EFI_END_ENTIRE_DEVICE_PATH_SUBTYPE;
+      ldp->length = sizeof (*ldp);
+      ldp = grub_efi_find_last_device_path (ddp);
+
+      if (GRUB_EFI_DEVICE_PATH_SUBTYPE (ldp) ==  GRUB_EFI_MAC_ADDRESS_DEVICE_PATH_SUBTYPE)
+	{
+	  grub_efi_mac_address_device_path_t *mac = (grub_efi_mac_address_device_path_t *) ldp;
+	  bp->hw_type = mac->if_type;
+	  bp->hw_len = sizeof (bp->mac_addr);
+	  grub_memcpy (bp->mac_addr, mac->mac_address, bp->hw_len);
+	}
+    }
+  else
+    {
+      grub_efi_ipv6_device_path_t *ipv6 = (grub_efi_ipv6_device_path_t *) ldp;
+
+      struct grub_net_dhcp6_packet *d6p;
+      struct grub_net_dhcp6_option *opt;
+      struct grub_net_dhcp6_option_iana *iana;
+      struct grub_net_dhcp6_option_iaaddr *iaaddr;
+
+      d6p = (struct grub_net_dhcp6_packet *)nb->tail;
+      err = grub_netbuff_put (nb, sizeof(*d6p));
+      if (err)
+	{
+	  grub_free (ddp);
+	  grub_netbuff_free (nb);
+	  return NULL;
+	}
+      d6p->message_type = GRUB_NET_DHCP6_REPLY;
+
+      opt = (struct grub_net_dhcp6_option *)nb->tail;
+      err = grub_netbuff_put (nb, sizeof(*opt));
+      if (err)
+	{
+	  grub_free (ddp);
+	  grub_netbuff_free (nb);
+	  return NULL;
+	}
+      opt->code = grub_cpu_to_be16_compile_time (GRUB_NET_DHCP6_OPTION_IA_NA);
+      opt->len = grub_cpu_to_be16_compile_time (sizeof(*iana) + sizeof(*opt) + sizeof(*iaaddr));
+
+      err = grub_netbuff_put (nb, sizeof(*iana));
+      if (err)
+	{
+	  grub_free (ddp);
+	  grub_netbuff_free (nb);
+	  return NULL;
+	}
+
+      opt = (struct grub_net_dhcp6_option *)nb->tail;
+      err = grub_netbuff_put (nb, sizeof(*opt));
+      if (err)
+	{
+	  grub_free (ddp);
+	  grub_netbuff_free (nb);
+	  return NULL;
+	}
+      opt->code = grub_cpu_to_be16_compile_time (GRUB_NET_DHCP6_OPTION_IAADDR);
+      opt->len = grub_cpu_to_be16_compile_time (sizeof (*iaaddr));
+
+      iaaddr = (struct grub_net_dhcp6_option_iaaddr *)nb->tail;
+      err = grub_netbuff_put (nb, sizeof(*iaaddr));
+      if (err)
+	{
+	  grub_free (ddp);
+	  grub_netbuff_free (nb);
+	  return NULL;
+	}
+      grub_memcpy (iaaddr->addr, ipv6->local_ip_address, sizeof(ipv6->local_ip_address));
+
+      opt = (struct grub_net_dhcp6_option *)nb->tail;
+      err = grub_netbuff_put (nb, sizeof(*opt) + uri_len);
+      if (err)
+	{
+	  grub_free (ddp);
+	  grub_netbuff_free (nb);
+	  return NULL;
+	}
+      opt->code = grub_cpu_to_be16_compile_time (GRUB_NET_DHCP6_OPTION_BOOTFILE_URL);
+      opt->len = grub_cpu_to_be16 (uri_len);
+      grub_memcpy (opt->data, uri_dp->uri, uri_len);
+
+      *use_ipv6 = 1;
+    }
+
+  grub_free (ddp);
+  return nb;
+}
+
 static void
 grub_efi_net_config_real (grub_efi_handle_t hnd, char **device,
 			  char **path)
@@ -361,6 +577,11 @@
     grub_efi_device_path_t *cdp;
     struct grub_efi_pxe *pxe;
     struct grub_efi_pxe_mode *pxe_mode;
+    grub_uint8_t *packet_buf;
+    grub_size_t packet_bufsz ;
+    int ipv6;
+    struct grub_net_buff *nb = NULL;
+
     if (card->driver != &efidriver)
       continue;
     cdp = grub_efi_get_device_path (card->efi_handle);
@@ -380,11 +601,21 @@
 	ldp = grub_efi_find_last_device_path (dp);
 	if (GRUB_EFI_DEVICE_PATH_TYPE (ldp) != GRUB_EFI_MESSAGING_DEVICE_PATH_TYPE
 	    || (GRUB_EFI_DEVICE_PATH_SUBTYPE (ldp) != GRUB_EFI_IPV4_DEVICE_PATH_SUBTYPE
-		&& GRUB_EFI_DEVICE_PATH_SUBTYPE (ldp) != GRUB_EFI_IPV6_DEVICE_PATH_SUBTYPE))
+		&& GRUB_EFI_DEVICE_PATH_SUBTYPE (ldp) != GRUB_EFI_IPV6_DEVICE_PATH_SUBTYPE
+		&& GRUB_EFI_DEVICE_PATH_SUBTYPE (ldp) != GRUB_EFI_URI_DEVICE_PATH_SUBTYPE))
 	  continue;
 	dup_dp = grub_efi_duplicate_device_path (dp);
 	if (!dup_dp)
 	  continue;
+
+	if (GRUB_EFI_DEVICE_PATH_SUBTYPE (ldp) == GRUB_EFI_URI_DEVICE_PATH_SUBTYPE)
+	  {
+	    dup_ldp = grub_efi_find_last_device_path (dup_dp);
+	    dup_ldp->type = GRUB_EFI_END_DEVICE_PATH_TYPE;
+	    dup_ldp->subtype = GRUB_EFI_END_ENTIRE_DEVICE_PATH_SUBTYPE;
+	    dup_ldp->length = sizeof (*dup_ldp);
+	  }
+
 	dup_ldp = grub_efi_find_last_device_path (dup_dp);
 	dup_ldp->type = GRUB_EFI_END_DEVICE_PATH_TYPE;
 	dup_ldp->subtype = GRUB_EFI_END_ENTIRE_DEVICE_PATH_SUBTYPE;
@@ -396,16 +627,31 @@
       }
     pxe = grub_efi_open_protocol (hnd, &pxe_io_guid,
 				  GRUB_EFI_OPEN_PROTOCOL_GET_PROTOCOL);
-    if (! pxe)
-      continue;
-    pxe_mode = pxe->mode;
+    if (!pxe)
+      {
+	nb = grub_efinet_create_dhcp_ack_from_device_path (dp, &ipv6);
+	if (!nb)
+	  {
+	    grub_print_error ();
+	    continue;
+	  }
+	packet_buf = nb->head;
+	packet_bufsz = nb->tail - nb->head;
+      }
+    else
+      {
+	pxe_mode = pxe->mode;
+	packet_buf = (grub_uint8_t *) &pxe_mode->dhcp_ack;
+	packet_bufsz = sizeof (pxe_mode->dhcp_ack);
+	ipv6 = pxe_mode->using_ipv6;
+      }
 
-    if (pxe_mode->using_ipv6)
+    if (ipv6)
       {
 	grub_net_configure_by_dhcpv6_reply (card->name, card, 0,
 					    (struct grub_net_dhcp6_packet *)
-					    &pxe_mode->dhcp_ack,
-					    sizeof (pxe_mode->dhcp_ack),
+					    packet_buf,
+					    packet_bufsz,
 					    1, device, path);
 	if (grub_errno)
 	  grub_print_error ();
@@ -414,8 +660,8 @@
       {
     inter = grub_net_configure_by_dhcp_ack (card->name, card, 0,
 					    (struct grub_net_bootp_packet *)
-					    &pxe_mode->dhcp_ack,
-					    sizeof (pxe_mode->dhcp_ack),
+					    packet_buf,
+					    packet_bufsz,
 					    1, device, path);
 
     if (inter != NULL)
@@ -441,6 +687,10 @@
 	  }
       }
       }
+
+    if (nb)
+      grub_netbuff_free (nb);
+
     return;
   }
 }
--- a/include/grub/efi/api.h
+++ b/include/grub/efi/api.h
@@ -876,6 +876,8 @@
   grub_efi_uint16_t remote_port;
   grub_efi_uint16_t protocol;
   grub_efi_uint8_t static_ip_address;
+  grub_efi_ipv4_address_t gateway_ip_address;
+  grub_efi_ipv4_address_t subnet_mask;
 } GRUB_PACKED;
 typedef struct grub_efi_ipv4_device_path grub_efi_ipv4_device_path_t;
 
@@ -939,6 +941,15 @@
 } GRUB_PACKED;
 typedef struct grub_efi_vlan_device_path grub_efi_vlan_device_path_t;
 
+#define GRUB_EFI_URI_DEVICE_PATH_SUBTYPE		24
+
+struct grub_efi_uri_device_path
+{
+  grub_efi_device_path_t header;
+  grub_efi_uint8_t uri[0];
+} GRUB_PACKED;
+typedef struct grub_efi_uri_device_path grub_efi_uri_device_path_t;
+
 #define GRUB_EFI_VENDOR_MESSAGING_DEVICE_PATH_SUBTYPE	10
 
 /* Media Device Path.  */
